PENDANT LOUDSPEAKER

━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━

(1) 기능

본 기기는 6.5인치 1개, 2.75인치 4개를 구성하여 200W rms 전력을 제공하고 펜던트 형태로 설치가 가능한 기기이어야 한다.

(2) 기기특성

System details

- LF transducer	: 165mm(6.5in) dual

voicecoilsubwoofer, stamped

basket,16Ω nominal impedance,

paper cone, paper dust cap, copper

wire, rubber surround

- HF transducer	: 4x 69.85mm (2.75in) full-range,

stamped basket, 16Ω nominal

impedance, hybrid

ceramic/neodymium magnetic

circuit, copper cap, paper cone,

inverted aluminum dust cap,

CC aluminum VC wire,

rubber surround

- Effective frequency range	: 40Hz – 20kHz

- Maxnoisevoltage	: 24.5V(rms)

- Sensitivity(dB)	: 86

- Coverage(‐6dB)	: 110°conical

- Directivity factor	: 6.0

- Directivity index(dB)	: 8dB

- Maximum continuous SPL(dB)	: 105

- Maximum peak SPL(dB)	: 111

- Recommended amplifier	: 25W per satellite

(with 1st order high-pass filter at

200Hz)

- Nominal Impedance	: 6Ω nominal

4.9Ω minimum @ 1.6kHz

- Crossover frequency	: 250Hz(2nd order low-pass +

3rd order highpassfilters)

- Tap power(70V/100V)	: 12.5, 25, 50, 100/25, 50, 100

- Port tuning	: 50Hz

- Input	: 4-pin male/female euroblockwith

pass-thru and locking screws

Enclosure details

- Enclosure material	: Injection-molded ABS

baffle and enclosure

- Grille material	: Stamped steel, perforated and

powdercoated

- Weight(net/shipping)	: 10.2Ib(22.5kg)/12.5Ib(27.6kg)

- Product dimensions(diameter x height)	: Ø 13.37 x 17.04in

(Ø339.7 x 433mm)

- Shipping dimensions(WxDxH)	: 21.06 x 17.52 x 17.13in

(535 x 445 x 435mm)

** AD-P.HALO 또는 동등 이상품 이어야 한다.