CEILING SUBWOOFER

━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━

(1) 기능

본 기기는 6.5인치 실링 서브우퍼로서 UL1480 및 UL2043 인증을 받은 기기이어야 한다.

(2) 기기특성

System details

- LF transducer	: 6.5"(165mm) dual voice-coil

weather treated paper cone woofer

- HF transducer	: N/A

- Effective frequency range	: 45Hz – 150Hz

- Rated noise power/voltage	: 100W/20V(rms)

- Sensitivity(dB)(Rated @ 1W, 1m)	: 86

- Coverage(‐6dB)	: 250

- Directivity factor	: 1.8

- Directivity index(dB)	: 1.5

- Maximum continuous SPL(dB)	: 100

- Maximum peak SPL(dB)	: 106

- Recommended amplifier	: 100W

- Transformer taps/Impedance	: Bypass: 4Ω

100W(70V); N/A(100V) Tap: 50Ω

50W(70V); 100W(100V) Tap: 100Ω

25W(70V); 50W(100V) Tap: 200Ω

12.5W(70V);25W(100V) Tap: 400Ω

- Connector	: Mono input: 4-pole euroblockwith

thru output Hi-pass mono output:

2x 4-pole Euroblockfor 4x satellites

Enclosure details

- Enclosure material	: ABS baffle on powder coated steel

back can

- Grille material	: Powder coated steel

- Ingress protection	: IP-34

- Operating environment	: Designed for indoor use

- Operating temperature range	: -20 to 50°C(-4 to 122 °F)

- Cutout dimension	: Ø 12in(Ø305mm)

- Weight(net/shipping)	: 19.2Ib(8.7kg)/11.9Ib(26.2kg)

- Product dimensions(diameter x height)	: Ø 13.4 x 10.4in(Ø340 x 263mm)

- Shipping dimensions(DxWxH)	: 21 x 21 x 15in

(533 x 533 x 381mm)

- Included mounting hardware	: C-ring and tile rails, rail screws,

3x Euroblockconnector,

cut-out template, grill

- Safety agency	: UL1480, UL2043, NFPA90,

NFPA70 suitable for use in air

handling spaces. ROHS,

CE compliant. Baffle meets

UL94-V0 and UL94-5VB

flamibilityrating; in accordance with

IEC60849 / EN60849 systems.

** AD-C.SUB 또는 동등 이상품 이어야 한다.