SURFACE LOUDSPEAKER

━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━

(1) 기능

본 기기는 2.75인치 스피커로서 X-Mount로 고정하여 유연하게 각도를 조정할 수 있는 기기이어야 한다.

(2) 기기특성

System details

- LF transducer	: N/A

- HF transducer	: 2.75in(70mm) weather treated

paper cone woofer

- Effective frequency range	: 150Hz – 20kHz

- Rated noise power/voltage	: 25W/20V(rms)

- Sensitivity(dB)(Rated @ 1W, 1m)	: 82

- Coverage(‐6dB)	: 155°conical

- Directivity factor	: 4.0

- Directivity index(dB)	: 6.0

- Maximum continuous SPL(dB)	: 90

- Maximum peak SPL(dB)	: 96

- Recommended amplifier	: 25W per satellite

(with 1st order high-pass filter at

200Hz)

- Impedance	: 16Ω

- Connector	: 2-pole euroblockconnectors

Enclosure details

- Enclosure material	: ABS

- Grille material	: Aluminum

- Ingress protection	: IP-34

- Operating environment	: Designed for indoor use

- Operating temperature range	: -20 to 50°C(-4 to 122 °F)

- Cutout dimension	: Ø 4.5in(Ø115mm)

- Weight(net/shipping)	: 0.95Ib(0.433kg)/TBD(pair packed)

- Product dimensions including wall bracket(HxWxD) : 3.6 x 3.5 x 5.4 in

(92.5 x 89 x 136 mm)

- Shipping dimensions(HxWxD)	: TBD(pair packed)

- Included mounting hardware	: X-Mount Mini ,

Euroblockconnector (pair packed)

- Safety agency	: ROHS, CE compliant.

** AD-S.SAT 또는 동등 이상품 이어야 한다.