SURFACE SUBWOOFER

━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━

(1) 기능

본 기기는 6.5인치 서브우퍼로서 Low-Z 모드로 모노 또는 스테레오 구성이 가능한 기기이어야 한다.

(2) 기기특성

System details

- LF transducer	: 6.5in(165mm) dual voice coil

weather treated paper cone woofer

- HF transducer	: N/A

- Effective frequency range	: 45Hz – 150Hz

- Rated noise power/voltage	: 100W/20V(rms)

- Sensitivity(dB)(Rated @ 1W, 1m)	: 86

- Coverage(‐6dB)	: Omni

- Directivity factor	: 1.58

- Directivity index(dB)	: 2.0

- Maximum continuous SPL(dB)	: 100

- Maximum peak SPL(dB)	: 106

- Recommended amplifier	: 100W

- Transformer taps/impedance	: 70V: 100, 50, 25,12.5W(mono only)

100V: 100, 50, 25W(mono only)

Bypass:4Ω mono or 8Ω+8Ω stereo

- Connector	: Hi-Z mono input: 4-pole

euroblockwith thru output

Low-Z input: 4-pole euroblock,

left(mono) and right

Hi-pass output: x2 4-Pole

euroblockfor x4 satellites

Enclosure details

- Enclosure material	: Vinyl wrapped medium density

fiberboard

- Port baffle/cover panel	: ABS

- Ingress protection	: N/A

- Operating environment	: Designed for indoor use

- Operating temperature range	: -20 to 50°C(-4 to 122 °F)

- Cutout dimension	: Ø 4.5in(Ø115mm)

- Weight(net/shipping)	: 23.6Ib(10.7kg)/13.94Ib(30.73kg)

- Product dimensions(HxWxD)	: 13.8 x 8.2 x 1.7in

(350 x 209 x 432mm)

- Shipping dimensions(HxWxD)	: 21.0 x 12.4 x 18.6in

(535 x 315 x 473mm)

- Included accessories	: V-wall bracket, 4x

Euroblockconnector, rear cover

panel, adhesive rubber feet

- Safety agency	: Transformer UL registered per

UL1876, ROHS, CE compliant

** AD-S.SUB 또는 동등 이상품 이어야 한다.