PENDANT LOUDSPEAKER

━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━

(1) 기능

본 기기는 2.75인치 스피커로서 UL1480 인증을 받은 기기이어야 한다.

(2) 기기특성

System details

- LF transducer	: N/A

- HF transducer	: 2.75in(70mm) weather treated

paper cone woofer

- Effective frequency range	: 150Hz – 20kHz

- Rated noise power/voltage	: 25W/20V(rms)

- Sensitivity(dB)(Rated @ 1W, 1m)	: 83

- Coverage(‐6dB)	: 155°conical

- Directivity factor	: 4.0

- Directivity index(dB)	: 6.0

- Maximum continuous SPL(dB)	: 90

- Maximum peak SPL(dB)	: 96

- Recommended amplifier	: 25W per satellite

(with 1st order high-pass filter at

200Hz)

- Impedance	: 16Ω

- Connector	: 2-pole euroblockconnectors

Enclosure details

- Enclosure material	: ABS

- Grille material	: Powder coated steel

- Ingress protection	: IP-34

- Operating environment	: Designed for indoor use

- Operating temperature range	: -20 to 50°C(-4 to 122 °F)

- Weight(net/shipping)	: 0.93Ib(0.420kg)/2.27Ib(1.03kg)

- Product dimensions(diameter x height)	: Ø 4.3 x 4.9in(Ø110 x 124mm)

- Shipping dimensions(HxWxD)	: 12.3 x 6.5 x 6in

(313 x 165 x 152mm)

- Included accessories	: Cable rigging,

1x euroblockconnector,

grille attached

- Safety agency	: UL1480

** AD-P.SAT 또는 동등 이상품 이어야 한다.