PENDANT SUBWOOFER

━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━

(1) 기능

본 기기는 6.5인치 서브우퍼로서 UL1480 인증을 받은 기기이어야 한다.

(2) 기기특성

System details

- LF transducer	: 6.5in(165mm) dual voice-coil

weather treated paper cone woofer

- HF transducer	: N/A

- Effective frequency range	: 50Hz – 150Hz

- Rated noise power/voltage	: 100W/20V(rms)

- Sensitivity(dB)(Rated @ 1W, 1m)	: 86

- Coverage(‐6dB)	: Omni

- Directivity factor	: 1.3

- Directivity index(dB)	: 1.2

- Maximum continuous SPL(dB)	: 100

- Maximum peak SPL(dB)	: 106

- Recommended amplifier	: 100W

- Transformer taps/Impedance	: Bypass:4 Ω

100W(70V); N/A(100 V) Tap: 50Ω

50W(70V); 100W(100V) Tap: 100Ω

25W(70V); 50W(100V) Tap: 200Ω

12.5W(70V);25W(100V) Tap: 400Ω

- Connector	: Mono input: 4-pole euroblockwith

thru output Hi-pass mono output:

2x 4-pole euroblockfor 4x satellites

Enclosure details

- Enclosure material	: ABS

- Grille material	: Powder coated steel

- Ingress protection	: IP-34

- Operating environment	: Designed for indoor use

- Operating temperature range	: -20 to 50°C(-4 to 122 °F)

- Weight(net/shipping)	: 17.53Ib(7.95kg)/21.8Ib(9.89kg)

- Product dimensions(diameter x height)	: Ø 13.6 x 14.1in(Ø346 x 359mm)

- Shipping dimensions(HxWxD)	: 17.1 x 17.1 x 17.1in

(435 x 435 x 435mm)

- Included accessories	: 2x cable rigging, 3x

euroblockconnector,

2x sealed input cover, grill

- Safety agency	: UL1480, transformer UL registered

per UL1876, ROHS, CE compliant.

** AD-P.SUB 또는 동등 이상품 이어야 한다.