LOUD SPEAKER

━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━

(1) 기능

본 기기는 5.25인치 2Way 천장형 스피커로 5.25인치 우퍼 드라이버와 1인치 우퍼  다습한 환경에 강한 폴리프로필렌 콘이 장착되어 있고 밀폐형 인클로저는 70Hz 이하의 저주파를 전달하는 데에 최적화되어 있어야 하며 우퍼와 선대칭으로 장착된 기존의 트위터 타입에서 자주 발생하던 간섭 현상을 줄이기 위해, 트위터는 우퍼의 중심부에서 약간 빗겨 장착이 되어 있어야 한다. 하이임피던스 용 트랜스포머가 장착되어 8옴 뿐 아니라 70V 및 100V로 변환하여 전관방송에도 적합한 기기이어야 한다.

(2) 기기특성
System Details

- HF transducer	: 1 in (25 mm) damped fabric dome

tweeter/1 in voice-coil, NdFeB magnet

- LF transducer	: 5.25 in (135 mm) paper cone woofer

1 in voice-coil, ferrite magnet

- Effective frequency range	: 65 – 20 kHz

- Rated noise power / voltage	: 100 W

- Broad-band sensitivity	: 86.3 dB SPL

- Coverage angle (-6 dB)	: 115°

- Directivity factor (Q)	: 6.9

- Directivity index	: 8.4 dB

- Maximum continuous SPL	: 106 dB

- Maximum peak SPL	: 116 dB

- Rated impedance	: 8 Ω

- Recommended amplifier power	: 300 W

- Transformer taps	: 70 V: 7.5, 15, 30, 60, bypass

100 V: n/a, 15, 30, 60, bypass

- Input connector type	: 4-pin Euroblock connector with

parallel output

- Enclosure material	: Painted ABS polymer

- Grille material	: Powder coated aluminum

Enclosure Details

- Ingress protection	: IP-54

- Operating environment	: Designed for indoor and outdoor use

- Testing	: The AD Series loudspeakers qualified

for outdoor use using the following

tests:

Salt fog: MIL-STD-810G

Method 509.5 for 100 hrs.

Humidity: MIL-STD-810G

Method 507.5,Natural cycle B2,

cyclic high RH for 7 days

High and low temperature: tested

according to QSC internal standards

between -20° and 50° C

- Operating Temperature Range	: -20 to 50 °C / -4 to 122 °F

- Net weight	: 9.92 lbs / 4.5 kg

- Product dimensions	: 11.26 x 6.88 X 6.85 in

(286 x 175 x 174 mm)

- Shipping weight	: 20.2 lbs / 9.2 kg (pair packed)

- Shipping dimensions	: 15.9" x 10.31" X 18.3“

(405 x 262 x 465mm) (pair packed)

- Included accessories	: X-Mount mounting system,

euroblock connector,

input panel cover

** AD-S5T 또는 동등 이상품 이어야 한다.