POWERED SUBWOOFER SPEAKER

━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━

(1) 기능

본 기기는 Active front-loaded 서브우퍼 시스템으로 Class D 앰프를 사용하며, 어레이로 플라잉하거나 그라운드 스택으로 사용할 수 있는 제품이어야 한다. Deep-Loud EQ 스위치를 통해 사용자는 저음 출력을 맞춤화하여 사용할 수 있고, 80Hz-125Hz에 대한 가변 로우 패스 필터를 컨트롤할 수 있어야 한다. 자작나무 합판 인클로저를 사용하고, 내구성이 뛰어난 ISO-flex 페인트 도장을 한 제품이어야 한다.

(2) 기기특성

- Frequency Range (-10 dB)	: 35 Hz - 125 Hz

- Maximum Peak SPL at 1 m	: 134 dB

- Nominal Amplifier Power (continuous)	: 1000 W

- Nominal Amplifier Power (peak)	: 2000 W

- Input Type	: Balanced

- Input Impeadance	: 20 kohms

- Input Sensitivity	: 3 V (+12 dBu)

- Audio Signal Input Connector	: 2 x Female XLR

- Audio Signal Loop Thru Connector	: 2 x Male XLR

- AC Output Connector	: powerCON NAC3FCB

- Current Draw 230 V / 115 V	: 2.2 A/4.4 A

- Enclosure Construction	: Birch Plywood

- Enclosure Geometry	: Rectangular

- Rigging	: M10 Rigging Points

- Finish	: ISO-flex Paint

- Color	: Black

- Dimensions ( H x W x D )	: 490 x 615 x 785 mm

19.3 x 24.2 x 30.9 in

- Net Weight	: 44.0 kg ( 97.0 lb )

** VANTEC-118A 또는 동등 이상품 이어야 한다.