POWERED SUBWOOFER SPEAKER

━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━

(1) 기능

본 기기는 ultra-low frequency 서버우퍼 시스템으로 6인치 보이스 코일이 장착된 2개의 21인치 스피커로 인상적인 60mm 피크 간 편위를 가지고 강력하고 제어된 저음을 재생할 수 있어야 한다. Class D 앰프를 사용하며 DASnet™을 통한 원격 모니터링 및 제어가 가능하여야 한다. 전면에 위치한 커넥터를 사용하여 카디오이드 구성을 할 때 쉽게 설치할 수 있어야 하며 고효율, 저소비 전력 범용 전원 공급 장치 PCF를 사용해야 한다. 자작나무 합판 인클로저를 사용하고, 내구성이 뛰어난 ISO-flex 페인트 도장을 한 제품이어야 한다.

(2) 기기특성

- Frequency Range (-10 dB)	: 28 Hz - 125 Hz

- Maximum Peak SPL at 1 m	: 145 dB

- Nominal Amplifier Power (continuous)	: 2 x 3400 W

- Nominal Amplifier Power (peak)	: 2 x 6800 W

- Input Type	: Balanced

- Input Impeadance	: 20 kohms

- Input Sensitivity	: 4.9 V (+16 dBu)

- Audio Signal Input Connector	: 1 x Female XLR

- Audio Signal Loop Thru Connector	: 1 x Male XLR

- Audio/Data Input Connector	: etherCON

- Control	: DASnet™

- Audio + Data Loop Thru Connector	: etherCON

- Current Draw 230 V / 115 V	: 9.2 A/18.4 A

- Enclosure Construction	: Birch Plywood

- Enclosure Geometry	: Rectangular

- Rigging System	: Ground Stackable Rigging points

- Finish	: ISO-flex Paint

- Color	: Black

- Dimensions ( H x W x D )	: 615 x 1,195 x 1,100 mm

24.2 x 47.0 x 43.3 in

- Net Weight	: 133.0 kg ( 293.3 lb )

** UX-221A 또는 동등 이상품 이어야 한다.