POWER AMPLIFIER

━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━

(1) 기능

본 기기는 파워 앰프로 입력 감도 및 작동 모드 (스테레오, 브릿지. 병렬 모드)를 선택할 수 있어야 한다. 듀얼 밸런스 XLR 입력을 가지며 출력 단락, 과부하 및 과열로부터 보호할 수 있어야 한다. 전면 LED를 통해 전원, 클립, 보호 및 신호를 표시 할 수 있고, 볼륨 컨트롤도 할 수 있어야 한다.

(2) 기기특성

- Power 8 Ohms, Both Channels Driven	: 2 x 1000 W

- Power 8 Ohms Bridged	: 2700 W

- Power 4 Ohms, Both Channels Driven	: 2 x 1350 W

- Amplifier Channels	: 2

- Frequency Response	: 20 Hz - 20 kHz, +0 – 1 dB

- Total Harmonic Distortion	: <0.5% , 20 Hz - 20 kHz

- Signal to Noise Ratio	: > 100 dB @ 20 Hz – 20 kHz

- Voltage gain	: 36 dB

- Damping Factor	: > 200 @ 10 Hz - 400 Hz

- Controls	: Power On/Off, Gain Pots

- Cooling	: Internal heat sinks with forced air:	Fan cooled

- Amplifier Protections	: Protection against short circuits,

no-load, on/off muting,

RF interference.

- LED Indicators	: Power, Protection, Signal, Clip

- Audio Signal Input Connector	: 2 x Female XLR

- Audio Signal Loop Thru Connector	: 2 x Male XLR

- Speaker Output Connector	: 2 x speakON

- Dimensions ( H x W x D )	: 88 x 482 x 227 mm

3.5 x 19.0 x 8.9 in

- Net Weight	: 19.5 kg ( 43.0 lb )

** PA-2700 또는 동등 이상품 이어야 한다.