POWERED LINEARRAY SPEAKER

━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━

(1) 기능

본 기기는 고급 라인어레이 시스템으로 tri-amplified Class D 앰프를 사용하며 Brickwall FIR 필터를 사용하여 강력한 DSP 기능을 가져야 한다. DASaim™으로 원격 SPL 레벨 제어 및 어레이 수직 방사 패턴의 Digital steering으로 어레이 시스템을 개별적으로 조정할 수 있어야 한다. DASnet™을 통한 원격 모니터링 및 제어가 가능하고, 간편한 리깅/스태킹을 위한 Quick 리그 시스템을 가지고 있어야 한다. 자작나무 합판 인클로저를 사용하고, 내구성이 뛰어난 ISO-flex 페인트 도장을 한 제품이어야 한다.

(2) 기기특성

- Frequency Range (-10 dB)	: 60 Hz - 20 kHz

- Horizontal Coverage (-6 dB)	: 90º

- Vertical Coverage	: Splay Dependent

- Maximum Peak SPL at 1 m	: 138 dB

- Nominal Amplifier Power LF (continuous)	: 1000 W

- Nominal Amplifier Power LF (peak)	: 2000 W

- Nominal Amplifier Power MF (continuous)	: 500 W

- Nominal Amplifier Power MF (peak)	: 1000 W

- Nominal Amplifier Power HF (continuous)	: 500 W

- Nominal Amplifier Power HF (peak)	: 1000 W

- Input Type	: Balanced

- Input Impeadance	: 20 kohms

- Input Sensitivity	: 6.2 V (+18 dBu)

- Audio Signal Input Connector	: 1 x Female XLR

- Audio Signal Loop Thru Connector	: 1 x Male XLR

- Audio/Data Input Connector	: etherCON

- Control	: DASnet™

- Audio + Data Loop Thru Connector	: etherCON

- AC Output Connector	: powerCON TRUE1

- Current Draw 230 V / 115 V	: 3.0 A/6.0 A

- Enclosure Construction	: Birch Plywood

- Enclosure Geometry	: Trapezoidal 3.5º

- Rigging System	: Integrated in box design

- IP Rating	: IP43

- Finish	: ISO-flex Paint

- Color	: Black

- Dimensions ( H x W x D )	: 320 x 1,012 x 520 mm

12.6 x 39.8 x 20.5 in

- Net Weight	: 78.0 kg ( 172.0 lb )

** AERO-40A 또는 동등 이상품 이어야 한다.