POWERED SUBWOOFER SPEAKER

━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━

(1) 기능

본 기기는 어레이 가능한 서버우퍼 시스템으로 Class D 앰프를 사용하며 DASnet™을 통한 원격 모니터링 및 제어, 로우 패스 필터 및 카디오이드 프리셋 선택이 가능하여야 한다. 전면에 위치한 커넥터를 사용하여 카디오이드 구성을 할 때 쉽게 설치할 수 있어야 하며, 초고속 리깅 하드웨어를 가지고 있어야 한다. 자작나무 합판 인클로저를 사용하고, 내구성이 뛰어난 ISO-flex 페인트 도장을 한 제품이어야 한다.

(2) 기기특성

- Frequency Range (-10 dB)	: 33 Hz - 120 Hz

- Maximum Peak SPL at 1 m	: 135 dB

- Nominal Amplifier Power (continuous)	: 1200 W

- Nominal Amplifier Power (peak)	: 2400 W

- Input Type	: Balanced

- Input Impeadance	: 20 kohms

- Input Sensitivity	: 6.2 V (+18 dBu)

- Audio Signal Input Connector	: 1 x Female XLR

- Audio Signal Loop Thru Connector	: 1 x Male XLR

- Control	: DASnet™

- AC Output Connector	: powerCON TRUE1

- Current Draw 230 V / 115 V	: 3.0 A/6.0 A

- Enclosure Construction	: Birch Plywood

- Enclosure Geometry	: Rectangular

- Rigging System	: Integrated in box design

- Finish	: ISO-flex Paint

- Color	: Black

- Dimensions ( H x W x D )	: 500 x 650 x 810 mm

19.7 x 25.6 x 31.9 in

- Net Weight	: 59.0 kg ( 130.1 lb )

** LX-118A 또는 동등 이상품 이어야 한다.