PASSIVE SPEAKER

━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━

(1) 기능

본 기기는 two-way passive full-range 시스템으로 회전 가능한 혼을 사용하여 수직 또는 수평으로 스피커를 설치할 수 있어야 한다. 자작나무 합판 인클로저를 사용하고, 내구성이 뛰어난 ISO-flex 페인트 도장을 한 제품이어야 한다. 후면 임피던스 멀티탭이 탑재되어 로우와 하이 임피던스 겸용으로 사용할 수 있어야 한다.

(2) 기기특성

- Frequency Range (-10 dB)	: 60 Hz - 20 kHz

- Horizontal Coverage (-6 dB)	: 90º

- Vertical Coverage	: 60º

- Nominal Impedance	: 16 ohms

- Transformer Taps 70 V	: 12.5 W, 25 W, 50 W, 100 W

- Transformer Taps 10 V	: 25 W, 50 W, 100 W

- RMS Power Handling	: 200 W

- Peak Power Handling	: 800 W

- On-axis Sensitivity 1W/1 m	: 93 dB SPL

- Maximum Peak SPL at 1 m	: 122 dB

- Audio Input Connector	: Covered Barrier Strip Terminals

- Audio Output Connector	: Covered Barrier Strip Terminals

- Enclosure Construction	: Birch Plywood

- Enclosure Geometry	: Trapezoidal

- Rigging	: M10 Rigging Points

- Finish	: ISO-flex Paint

- Color	: White

- Dimensions ( H x W x D )	: 550 x 195 x 260 mm

21.7 x 7.7 x 10.2 in

- Net Weight	: 10.0 kg ( 22.1 lb )

** ARTEC-326-TW 또는 동등 이상품 이어야 한다.