NETWORK AUDIO I/O EXPANDER

━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━

(1) 기능

본 기기는 네트워크 오디오 I/O 확장기로 Q-SYS 시스템의 기능을 확장하고 네트워크로 연결되지 않은 오디오 장치와의 상호 운용성을 간소화할 수 있어야 한다. 처리 하드웨어에서 로컬 I/O를 분리함으로써 원하는 토폴로지를 지원하기 위해 쉽게 확장이 가능한 모듈형 네트워크 I/O 제품이어야 한다. 4개의 마이크/라인 입력을 가지며, 48VDC 팬텀 전원을 사용할 수 있어야 한다. PoE(Power over Ethernet)를 지원하고 단일 네트워크 실행에서 최대 4개의 확장기를 데이지 체인 방식으로 연결하여 더 적은 수의 네트워크 포트를 사용할 수 있어야 한다. 표면 또는 1/4 너비의 1U 사이즈 랙 장착이 가능하여야 한다.

(2) 기기특성

Connectivity	: Four (4) mic/line inputs

Mic/Line Inputs

- Maximum input level	: +24 dBu

- Preamplifier gain range	: 0 dB to 60 dB

- Phantom power	: +48 VDC

- Equivalent Input Noise	: < -120 dBu, no weighting

@ 20 Hz to 20 kHz

- Input to input crosstalk @ 1 kHz	: > 85 dB

Input Dynamic Range

- @ +24 dBu sensitivity	: > 105 dB

- @ +10 dBu sensitivity	: > 100 dB

- @ -10 dBu sensitivity	: > 95 dB

- @ -36 dBu sensitivity	: > 80 dB

- Input impedance	: 5 kΩ single-ended, 10 kΩ balanced

Line Outputs

- Sample rate	: 48 kHz

- Bit Depth	: 24 bit

Other Connectors

- External power supply	: 24 VDC nominal, 2.5 A on Euro

connector with second connector for

daisy-chaining (QIO-PSU power

supply sold separately)

- LAN (PoE)	: Gigabit LAN connection for Q-LAN,

PoE

- PoE specification	: Conforms to IEEE 802.3af Type 1

- LAN (Thru)	: Ethernet daisy-chaining

General

- Dimensions ( D x W x H )	: 8.5 x 4.25 x 1.59 in

(215.9 x 108 x 40.4 mm)

- Weight	: 1.72 lb (0.78 kg)

** QIO-ML4i 또는 동등 이상품 이어야 한다.