NETWORK AUDIO I/O EXPANDER

━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━

(1) 기능

본 기기는 네트워크 오디오 I/O 확장기로 Q-SYS 시스템의 기능을 확장하고 네트워크로 연결되지 않은 오디오 장치와의 상호 운용성을 간소화할 수 있어야 한다. 처리 하드웨어에서 로컬 I/O를 분리함으로써 원하는 토폴로지를 지원하기 위해 쉽게 확장이 가능한 모듈형 네트워크 I/O 제품이어야 한다. 4개의 라인 출력을 가지며, PoE(Power over Ethernet)를 지원하고 단일 네트워크 실행에서 최대 4개의 확장기를 데이지 체인 방식으로 연결하여 더 적은 수의 네트워크 포트를 사용할 수 있어야 한다. 표면 또는 1/4 너비의 1U 사이즈 랙 장착이 가능하여야 한다.

(2) 기기특성

Connectivity	: Four (4) line outputs

Line Outputs

- Output audio range level	: -36 dBu to +24 dBu

- Output dynamic range	: 108 dB

- Output to output crosstalk @ 1 kHz	: > 85 dB

- Output Impedance	: 150 Ω to 300 Ω

- Sample rate	: 48 kHz

- Bit Depth	: 24 bit

Other Connectors

- External power supply	: 24 VDC nominal, 2.5 A on Euro

connector with second connector for

daisy-chaining (QIO-PSU power

supply sold separately)

- LAN (PoE)	: Gigabit LAN connection for Q-LAN,

PoE

- PoE specification	: Conforms to IEEE 802.3af Type 1

- LAN (Thru)	: Ethernet daisy-chaining

General

- Dimensions ( D x W x H )	: 8.5 x 4.25 x 1.59 in

(215.9 x 108 x 40.4 mm)

- Weight	: 1.72 lb (0.78 kg)

** QIO-L4o 또는 동등 이상품 이어야 한다.