NETWORK SERIAL I/O EXPANDER

━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━

(1) 기능

본 기기는 네트워크 SERIAL 확장기로 Q-SYS 시스템의 기능을 확장하여 SERIAL 연결을 통해 네트워크로 연결되지 않은 제어 장치와의 상호 운용성을 간소화할 수 있어야 한다. 처리 하드웨어에서 로컬 I/O를 분리함으로써 원하는 토폴로지를 지원하기 위해 쉽게 확장이 가능한 모듈형 네트워크 I/O 제품이어야 한다. 양방향 RS232 직렬 포트 4개를 가지며, PoE(Power over Ethernet)를 지원하고 단일 네트워크 실행에서 최대 4개의 확장기를 데이지 체인 방식으로 연결하여 더 적은 수의 네트워크 포트를 사용할 수 있어야 한다. 표면 또는 1/4 너비의 1U 사이즈 랙 장착이 가능하여야 한다.

(2) 기기특성

Serial Ports

- RS-232 / RS-485 / RS-422	: One (1) port, configurable protocol,

baud rate, and flow control

- RS232	: Three (3) port, configurable protocol,

baud rate, and flow control

Other Connectors

- External power supply	: 24 VDC nominal, 2.5 A on Euro

connector with second connector for

daisy-chaining (QIO-PSU power

supply sold separately)

- LAN (PoE)	: Gigabit LAN connection for Q-LAN,

PoE

- PoE specification	: Conforms to IEEE 802.3af Type 1

- LAN (Thru)	: Ethernet daisy-chaining

General

- Dimensions ( D x W x H )	: 5.5 x 4.25 x 1.59 in

(139.7 x 108 x 40.4 mm)

- Weight	: 1.18 lb (0.54 kg)

** QIO-S4 또는 동등 이상품 이어야 한다.