PASSIVE SPEAKER

━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━

(1) 기능

본 기기는 two-way passive 시스템으로 유럽 EN54-24 음성 경보 시스템 인증 제품으로 Weather Resistant에 적합한 IP56 등급을 받아 야외에서 사용할 수 있는 제품이어야 한다.

자작나무 합판 인클로저를 사용하고, 커버 노출을 위한 CX 버전으로 두꺼운 ISO-FLEX 폴리우레아 코팅으로 보호되어 있어야 한다. 70V/100V로 하이 임피던스 선택을 할 수 있어야 한다.

(2) 기기특성

- Frequency Range (-10 dB)	: 76 Hz - 20 kHz

- Horizontal Coverage (-6 dB)	: 80º

- Vertical Coverage	: 80º

- Nominal Impedance	: 133 ohms

- Transformer Taps 70 V	: 37 W

- Transformer Taps 100 V	: 75 W

- RMS Power Handling	: 75 W

- Peak Power Handling	: 300 W

- On-axis Sensitivity 1W/1 m	: 93 dB SPL

- Maximum Peak SPL at 1 m	: 118 dB

- Audio Input Connector	: Covered Barrier Strip Terminals

- Audio Output Connector	: Covered Barrier Strip Terminals

- Enclosure Construction	: Birch Plywood

- Enclosure Geometry	: Trapezoidal

- Rigging	: M10 Rigging Points

- Finish	: ISO-flex Paint

- Color	: Black

- IP Rating	: IP56

- Dimensions ( H x W x D )	: 550 x 230 x 270 mm

21.7 x 9.1 x 10.6 in

- Net Weight	: 11.0 kg ( 24.5 lb )

** WR-8826-TCX 또는 동등 이상품 이어야 한다.