POWERED SPEAKER

━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━

(1) 기능

본 기기는 Two-way bi-amp ribbon line source array SR system으로 3400W의 총 시스템 전력 피크를 가지며 Dante 이더넷 오디오 네트워크 입력 또는 아날로그 XLR 입력을 할 수 있어야 한다. 간편한 수직 커버리지 구성을 위한 Modular Line Array System™으로 FlyQWIK™ 하드웨어 리깅 시스템을 통해 직선 배열 구성 또는 다양한 각도 옵션을 시스템에서 쉽게 조정할 수 있어야 한다.

(2) 기기특성

- DSP On-Board	: Yes

- Networked Audio	: Yes (Dante)

- Network Control	: Yes

- Input Connectors	: 1 x XLR & 2 x RJ45

- Output Connectors	: 1 x XLR

- Speaker Configuration	: Line Array Module 2-way

- Speaker Type	: Powered

- Power RMS	: System – 850 W

(LF – 500 W & HF – 350 W)

- Power Program	: System – 1,700 W

(LF – 1,000 W & HF – 700 W)

- Power Peak	: System – 3,400 W

(LF – 2,000 W & HF – 1,400 W)

- Sensitivity (1W/1m)	: LF – 97 dB & HF – 101 dB

- Maximum SPL	: LF – 130 dB & HF – 130 dB

- Coverage (H x V)	: 90° x 15°

- Speaker Frequency Response	: 100 Hz – 20 Hz (±3 dB)

- Suspension Points	: FlyQWIK Flying Hardware

- Enclosure Material	: Baltic Birch Plywood

- Dimensions ( H x W x D )	: 384 x 689 x 426 mm

- Net Weight	: 34.10 kg

** Versarray™Pro112 또는 동등 이상품 이어야 한다.