PASSIVE SPEAKER

━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━

(1) 기능

본 기기는 Two-way bi-amp ribbon line source array SR system으로 1000W의 프로그램 파워를 가지는 12인치 라인어레이 스피커이어야 한다. 중소형 장소의 모듈식 커버리지를 제공하도록 설계되었으며, 네오 마그넷과 합성소재 샌드위치 리본이 있는 리본 트위터로 구성되어야 한다. FlyQWIK™ 하드웨어 리깅 시스템을 통해 직선 배열 구성 또는 다양한 각도 옵션을 시스템에서 쉽게 조정할 수 있어야 한다.

(2) 기기특성

- Speaker Configuration	: Line Array Module 2-way

- Speaker Type	: Non-Powered

Crossover Modes	: Bi-amp

- Power RMS	: LF – 500 W & HF – 120 W

- Power Program	: LF – 1,000 W & HF – 240 W

- Power Peak	: LF – 2,000 W & HF – 480 W

Nominal Impedance	: LF: 8 Ω & HF: 16 Ω

- Sensitivity (1W/1m)	: LF – 97 dB & HF – 101 dB

- Maximum SPL	: LF – 130 dB & HF – 128 dB

- Speaker Frequency Response	: 100 Hz – 20 Hz (±3 dB)

Coverage (H x V)	: 90° x 15°

- Input Connectors	: 2 x Neutrik® Speakon® NL4

- Suspension Points	: FlyQWIK Flying Hardware

- Enclosure Material	: Baltic Birch Plywood

- Dimensions ( H x W x D )	: 384 x 689 x 426 mm

- Net Weight	: 30.00 kg

** Versarray™112 MKIII 또는 동등 이상품 이어야 한다.