INTEGRATED DIGITAL SIGNAL PROCESSOR

━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━

(1) 기능

본 기기는 중앙 집중식 또는 에지 처리 배포 아키텍처 설계에 사용하도록 고안된 완전히 통합된 오디오, 비디오 및 제어 프로세서로 Q-SYS OS를 엔터프라이즈급 Dell COTS 서버 하드웨어와 결합하여 광범위한 대규모 확장을 위한 솔루션을 제공할 수 있어야 한다. 기본적으로 DiffServ 서비스 품질, IGMP, IEEE 1588-2008(PTPv2) 정밀 시간 프로토콜, 플로팅을 통한 UDP/IP 오디오 및 비디오 전송을 사용하여 다양한 네트워크 인프라 제조업체에서 제공하는 표준 기가비트 이더넷 인프라에서 작동할 수 있어야 한다. Q-LAN 또는 AES67 형식의 256 x 256 네트워크 오디오 채널과 64 x 64 미디어/WAN 스트리밍 용량, 64x VoIP 소프트폰 인스턴스를 제공할 수 있어야 한다. 8 x 8 소프트웨어 기반 Dante 네트워크 오디오 채널이 포함되어야 하며, Dante 기능 라이센스를 사용하면 최대 128 x 128까지 확장이 가능하여야 한다. 480GB 크기의 미디어 파일 저장용 SSD가 내장되어 있으며 4채널 음원 녹음이 가능하고, 16개의 멀티트랙을 재생을 할 수 있으며 옵션 기능 라이선스 사용시 최대 128개 채널로 확장할 수 있어야 한다. 터치스크린 컨트롤러, 네트워크로 연결된 오디오 I/O 확장기, 회의실 카메라 등 연동 가능한 네트워크 AV장비를 통하여 영상회의 또는 음향영상 시스템 송수신이 가능하여야 한다. 여러 회의 공간을 위한 중앙 집중식 처리뿐만 아니라 대규모 장소에 이르기까지 맞춤형 시스템을 구축할 수 있어야 한다.

(2) 기기특성

[ Hardware ]

- Platform	: Dell PowerEdge R250

- Power	: 1x universal input,

450 W PSU module

- LAN	: 4x 1000 Mbps ports

(2x Q-SYS Multimedia, 2x Q-SYS Aux)

- iDRAC	: 1x dedicated 1000 Mbps iDRAC v9,

basic license

- RS232	: 1x DB-9 RS-232 port (rear panel),

16550-compliant

- Ventilation	: Forced air – front intake,

rear exhaust

- Additional info	: Refer to Dell Specification Sheet and

Technical Guide

[ Control and Indicators ]

- Front	: Power button

ID button and indicator

(blinks when enabled from

Q-SYS Designer Software)

LCD display with navigation buttons

(displays Q-SYS Core hostname or

Core IP address)

- Rear	: ID button and indicator

(blinks when enabled from

Q-SYS Designer Software)

[ Q-SYS Capacities_Base features ]

- DSP processing power	: 16x

(relative to Q-SYS Core Nano)

- Network audio I/O (Q-LAN / AES67)	: 256 x 256

- AEC Channels (at 200 ms tail length)	: 64

- WAN / media streaming channels	: 64 x 64

- Q-SYS NM-T1 capacity	: 14

- Dante network I/O	: 8 x 8 included (up to 128 x 128

with Software-based Dante feature

license; Dante utilization subtracts

from Q-LAN capacity

- VoIP softphones	: 64

- Audio recording / playback	: 4 channels recording / 16 channels

playback, expandable up to 128

channels playback with

optional license

- Media drive	: 480 GB (approximately 440 GB

available for user media)

[ Packaging and Accessories ]

- Product dimensions (L x W x H)	: 23.56 x 18.98 x 1.69 in

(598.4 x 482.1 x 42.9 mm)

- Product weight	: 35 lbs (15.88 kg)

** CORE 610 또는 동등 이상품 이어야 한다.