NETWORK CEILING SPEAKER

━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━

(1) 기능

본 기기는 선명한 음성과 음악 재생을 제공하는 네트워크 PoE 스피커로 천장 장착형 인클로저에 4인치 전대역 드라이버를 갖추고 있어야 한다. Powered-over-Ethernet을 사용하여 단일 케이블을 통해 전원, 데이터 및 제어가 가능하고, 전체 하드웨어 설치 공간을 줄일 수 있어야 한다. Q-SYS Designer 소프트웨어 및 Q-SYS Reflect Enterprise Manager를 통한 포괄적인 관리가 가능하고, 스피커 보이싱(Intrinsic Correction™)을 통합하여 튜닝 과정을 단순화하여 제공할 수 있어야 한다. Q-SYS가 제공하는 드래그 앤 드롭 통합 및 간단한 제어 기능을 활용할 수 있어야 한다.

(2) 기기특성

- Loudspeaker type	: Network PoE ceiling-mount

loudspeaker for Q-SYS

- Driver	: 4-in (101.6 mm) full-range,

paper cone woofer, ferrite magnet

- Effective frequency range	: 100 Hz to 20 kHz

- Rated noise power / voltage (W rms)	: 12 W (PoE), 24 W (PoE+)

- Rated coverage	: 120°

- Directivity factor	: 3.8

- Directivity index	: 5.8 dB

- Maximum continuous SPL	: 94 dB (PoE), 97 dB (PoE+)

- Maximum peak SPL	: 108 dB (PoE), 111 dB (PoE+)

- Input connector type	: RJ45, Q-LAN

- Power requirements	: PoE (Type 1 Class 4) or

PoE+ (Type 2 Class 4)

- Enclosure material	: ABS baffle on powder steel back can

- Grille material	: Powder coated steel

Ingress protection	: IP34

- Operating temperature range	: 10° to 40° C

- Net weight	: 3.5 lbs (1.6 kg)

- Product dimension (diameter x height)	: 8.46 x 4.13 in

(215 x 105 mm)

** NL-C4 또는 동등 이상품 이어야 한다.