NETWORK SOUND BAR SPEAKER

━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━

(1) 기능

본 기기는 선명한 음성과 음악 재생을 제공하는 Two-way 네트워크 PoE 사운드바로 수평 및 수직 장착을 지원하여야 한다. Powered-over-Ethernet을 사용하여 단일 케이블을 통해 전원, 데이터 및 제어가 가능하고, 전체 하드웨어 설치 공간을 줄일 수 있어야 한다. Q-SYS Designer 소프트웨어 및 Q-SYS Reflect Enterprise Manager를 통한 포괄적인 관리가 가능하고, 스피커 보이싱(Intrinsic Correction™)을 통합하여 튜닝 과정을 단순화하여 제공할 수 있어야 한다. Q-SYS가 제공하는 드래그 앤 드롭 통합 및 간단한 제어 기능을 활용할 수 있어야 한다.

(2) 기기특성

- Loudspeaker type	: Network PoE soundbar for Q-SYS

- LF transducer	: 3.5-in (88.9 mm) paper cone woofer

- HF transducer	: 0.75-in (19.05 mm)silk dome tweeter

- Effective frequency range	: 110 Hz - 20 kHz

- Rated noise power	: 12 W (PoE), 24 W (PoE+)

- Rated coverage	: 150° horizontal, 160° vertical

(1 kHz - 10 kHz)

- Directivity factor	: 2.7

- Directivity index	: 4.2 dB

- Maximum continuous SPL	: 90 dB (PoE), 93 dB (PoE +)

- Maximum peak SPL	: 106 dB (PoE), 107 dB (PoE +)

- Input connector type	: RJ45

- Power requirements	: PoE (Type 1 Class 3) or

PoE+ (Type 2 Class 4)

- Power consumption	: 12 W maximum (PoE)

24 W maximum (PoE+)

- Enclosure material	: ABS

- Grille material	: Powder-coated steel

- Operating temperature range	: 10° to 40° C (50° to 104° F)

- Net weight	: 3.86 lbs (1.75 kg)

- Product dimensions	: 20.4 x 3.97 x 2.87 in

(518.1 x 101 x 73 mm)

** NL-SB42 또는 동등 이상품 이어야 한다.