POWER AMPLIFIER

━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━

(1) 기능

본 기기는 4채널 파워 앰프로 4옴에서 채널당 2000W를 제공하여야 한다. 스테레오 또는 브릿지 모드를 선택하거나 전면 LED를 통해 전원, 보호 및 출력 신호 레벨 확인 및 볼륨 컨트롤을 할 수 있어야 한다. Dante 네트워크 오디오 연결도 할 수 있어야 한다. (옵션)

(2) 기기특성

- Power 8 Ohms, Both Channels Driven	: 4 x 1000 W

- Power 8 Ohms Bridged	: 4000 W

- Power 4 Ohms, Both Channels Driven	: 4 x 2000 W

- Power 4 Ohms Bridged	: 4000 W

- Amplifier Channels	: 4

- Output Circuitry	: Class D

- Frequency Response	: 0.5 dB (20 Hz – 20 kHz)

- Total Harmonic Distortion	: < 0.2 %

- Input Impeadance	: 20 kohms

- Voltage gain	: 32 dB

- Damping Factor	: > 400

- Controls	: Power On/Off, Gain Pots

- Cooling	: Front-to-Back

- Amplifier Protections	: Protection Present , Short Circuit,

DC Output, Temperature

- LED Indicators	: Power On, Channel Output Level,	Channel Linked, Protection,

Bridged Pairs, Standby,

Analogue Audio, Network Audio

- Audio Signal Input Connector	: 4 x Female XLR

- Speaker Output Connector	: 4 x speakON

- Dimensions ( H x W x D )	: 88 x 485 x 425 mm

3.5 x 19.0 x 16.7 in

- Net Weight	: 10.1 kg ( 22.2 lb )

** DX-80-230 또는 동등 이상품 이어야 한다.