NETWORK POWER AMPLIFIER

━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━

(1) 기능

본 기기는 4채널 파워 앰프로 4옴에서 채널당 2700W를 제공하여야 한다. USB를 통해 PC에 연결하여 원격제어를 하거나, LCD 창으로 프리셋 및 정보를 확인할 수 있어야 한다. MUTE 키로 입력 또는 출력 채널을 음소거할 수 있고, 전면 LED를 통해 전원, 보호 및 출력 신호 레벨 확인을 할 수 있어야 한다. Ethernet, GPIO, RS485 Port를 통해 앰프를 제어하고,  Dante 네트워크 오디오 연결도 할 수 있어야 한다.

(2) 기기특성

- Power 8 Ohms, Both Channels Driven	: 4 x 1400 W

- Power 8 Ohms Bridged	: 5400 W

- Power 4 Ohms, Both Channels Driven	: 4 x 2700 W

- Power 4 Ohms Bridged	: 7000 W

- Amplifier Channels	: 4

- Output Circuitry	: Class D

- Frequency Response	: 0.5 dB (20 Hz – 20 kHz)

- Total Harmonic Distortion	: < 0.1 %

- Input Impeadance	: 20 kohms

- Voltage gain	: 32 dB

- Damping Factor	: > 400

- Controls	: Power On/Off, Channel Mute,

Rotary Encoder, Edit Keys,

Bank Keys, Navigation Keys

- Cooling	: Front-to-Back

- Amplifier Protections	: Protection Present , Short Circuit,

DC Output, Temperature

- LED Indicators	: LCD SCreen, Power On,

Channel Output Level,

Channel Linked, Protection,

Bridged Pairs, Standby,

Network Audio, Remote Control,

Digital In

- Audio Signal Input Connector	: 4 x Female XLR

- Audio Signal Loop Thru Connector	: 4 x Male XLR

- Speaker Output Connector	: 4 x speakON

- Dimensions ( H x W x D )	: 88 x 485 x 425 mm

3.5 x 19.0 x 16.7 in

- Net Weight	: 10.9 kg ( 24.0 lb )

** DX-100I-230 또는 동등 이상품 이어야 한다.