POWER AMPLIFIER

━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━

(1) 기능

본 기기는 파워 앰프로 입력 감도 및 작동 모드 (스테레오, 브릿지. 병렬 모드)를 선택할 수 있어야 한다. XLR 입력을 가지며 단락, 과부하 및 과열로부터 보호할 수 있어야 한다. 전면 LED를 통해 전원, 클립, 보호 및 신호를 표시 할 수 있고, 볼륨 컨트롤도 할 수 있어야 한다.

(2) 기기특성

- Rated Power Bridge 4 Ohms	: 3600 W

- Rated Power (2 x 2 Ohms)	: 2700 W per channel

- Rated Power (2 x 4 Ohms)	: 1800 W per channel

- Rated Power (2 x 8 Ohms)	: 1200 W per channel

- Rated Power (1 x 2 Ohms)	: 2800 W

- Rated Power (1 x 4 Ohms)	: 1900 W

- Rated Power (1 x 8 Ohms)	: 1280 W

- Minimum Load Impedance	: 2 Ohms

- Frequency Response	: 20 Hz- 20 kHz; +0, -1dB at 1watt

- T. H. D (2 x 8 Ohms)	: <0.1% @ 880 watts per channel

from 20 Hz to 20 kHz

- Damping Factor (8 Ohms)	: > 150:1 @20 Hz - 1 kHz at 8 ohms

- Phase Response	: +6 to -12 degrees form

20 Hz to 20 kHz

- Input Sensitivity	: 0.775V,1.0V, 1.44V +/-3%

- Input Impedance	: 15 k ohms, balanced

- Cooling	: Two back panel temperature

dependantvariable speed

80mm DC fan

- Indicator LEDs	: 1 PROT, 1 Clip (automatic clip

limiting), 1 -10dB ,

1 Signal presence, 1 Power status

- Protection	: Thermal, DC, turn-on bursts,

subsonic, incorrect loads

- Dimensions ( H x W x D )	: 88 x 485 x 475 mm

- Net Weight	: 24.8 kg

** CA2 18 또는 동등 이상품 이어야 한다.