POWER AMPLIFIER

━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━

(1) 기능

본 기기는 파워 앰프로 채널당 구성 가능한 70V, 100V, 4 또는 8Ω 모드에서 정격 전력으로 작동할 수 있어야 한다. 각 채널에는 제어 전압 입력이 포함되어 있어 외부 게인 제어가 가능하며, 각 채널의 결함 출력을 통해 앰프를 다른 모니터링 시스템에 연결할 수 있어야 한다. 클리핑 시작 시 게인을 자동으로 줄여 앰프 및 부하 손상을 방지하는 ACL™(Active Clip Limiting)과 부하 전류를 모니터링하여 과부하로부터 보호하는 IGM™(Instantaneous Gain Modulation)이 포함되어 있어야 한다.

(2) 기기특성

- Channels (Input)	: 4CH

- Channels (Output)	: 4CH

- Networked Audio	: Optional (CobraNet or Dante)

- Network Control	: Yes

- Power per Channel @ 4 Ω	: 1,250 W

- Power per Channel @ 8 Ω	: 1,250 W

- Power per Channel @ 70V	: 1,250 W

- Power per Channel @ 100V	: 1,250 W

- Topology	: Class D

- Minimum Load Impedance	: 4 Ω

- Frequency Response	: +0.8/-0.5 dB, 10 Hz – 22 kHz

- Input Connectors	: 4 x 3-pin Euro Connector

- Output Connectors	: 4 x 2-pin Barrier Strips

- Expansion-/Extension Card Slot	: Yes

- Rack Mount (19")	: Yes (2U)

- Dimensions ( H x W x D )	: 88 x 483 x 516 mm

- Net Weight	: 9.98 kg

** CKd1204 또는 동등 이상품 이어야 한다.