PASSIVE SPEAKER

━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━

(1) 기능

본 기기는 two-way long-throw 시스템으로 Horn을 탑재한 12인치 스피커이어야 한다. 회전

가능한 혼을 가지며 야외 설치가 가능하도록 제작된 IP54 제품으로, 스위치로 Passive 또는 Biamp 모드를 선택할 수 있어야 한다. 자작나무 합판 인클로저를 사용하고, 유리섬유 마감을 한 제품이어야 한다.

(2) 기기특성

- Frequency Range (-10 dB)	: 80 Hz - 18 kHz

- Horizontal Coverage (-6 dB)	: 90º

- Vertical Coverage	: 50º

- Nominal Impedance	: Passive: 8 ohms

- Nominal Impedance MF	: 8 ohms

- Nominal Impedance HF	: 8 ohms

- RMS Power Handling	: Passive: 400 W

- RMS Power Handling HF	: 150 W

- RMS Power Handling MF	: 400 W

- Peak Power Handling	: Passive: 1600 W

- Peak Power Handling MF	: 1600 W

- Peak Power Handling HF	: 400 W

- On-axis Sensitivity 1W/1 m	: Passive: 109 dB SPL

- On-axis Sensitivity 1W/1 m MF	: 109 dB SPL

- On-axis Sensitivity 1W/1 m HF	: 109 dB SPL

- Maximum Peak SPL at 1 m	: Passive: 141 dB

- Maximum Peak SPL at 1 m MF	: 141 dB

- Maximum Peak SPL at 1 m HF	: 137 dB

- Audio Input Connector	: 1 x speakON NL4

Covered Barrier Strip Terminals

- Audio Output Connector	: 1 x speakON NL4

Covered Barrier Strip Terminals

- Enclosure Construction	: Birch Plywood

- Enclosure Geometry	: Trapezoidal

- Rigging	: M10 Rigging Points

- Finish	: Fiberglass

- Color	: Black

- IP Rating	: IP54

- Dimensions ( H x W x D )	: 990 x 685 x 605 mm

39.0 x 27.0 x 24.0 in

- Net Weight	: 56.0 kg ( 123.5 lb )

** HQ-112.95-DX 또는 동등 이상품 이어야 한다.