NETWORK TOUCH SCREEN CONTROLLER

━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━

(1) 기능

본 기기는 네트워크 터치 스크린 컨트롤러로 24비트 컬러 디스플레이를 갖춘 PCAP (Projective Capacitive) 멀티 터치 표면을 가지고 있어야 한다. 1920 x 1200px, 380Nits(밝기)의 고해상도 디스플레이로 PoE(Power over Ethernet)를 지원해 단일 케이블로 설치가 가능하여야 한다. 손쉬운 드래그 앤 드롭 인터페이스로 사용자가 원하는 시스템의 제어 부분을 UCI에 구성하여 제어가 가능하여야 한다. 벽에 설치하여 사용하거나 테이블에 고정하여 사용할 수 있고, 세로 또는 가로 방향으로 장착이 가능하여야 한다.

(2) 기기특성

Display

- Type	: Projective capacitive (PCAP)

multi-touch technology,

high-resolution 24-bit color display

- Panel dimensions (WHD)	: 253.2 x 158.5 x 39.1 mm

- Viewable screen dimensions (diagonal)	: 10.07 in (255.8 mm)

- Resolution	: 1920 x 1200 px

- Aspect ratio	: 16:10

- Contrast ratio	: 800:1

- Brightness	: 380 Nits

- Customizable LED status indicators	: Yes

- Panel orientation	: Landscape / portrait

- Wall-mountable	: Yes (accessories included)

- Table top	: Optional table top stand accessory,

supports landscape orientation only

Sensors

- Ambient light sensor	: Yes

- Proximity detection (wake on approach)	: Yes

I/O

- LAN (1x RJ45)	: 1 Gbps

- USB 3.1 (1x Type-C)	: Yes (for future use)

Power

- Power over Ethernet	: PoE+ Class 4

Weight

- Product weight (net)	: 33.4 oz (947 g)

** TSC-101-G3 또는 동등 이상품 이어야 한다.