LANDSCAPE SPEAKER

━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━

(1) 기능

본 기기는 IP55의 등급을 가진 스피커로 내구성이 뛰어난 폴리프로필렌과 유리 섬유 구조 및 스테인리스 스틸 하드웨어를 갖추어 장기간의 실외 노출을 견딜 수 있도록 제작되어야 한다. 볼라드 디자인으로 야외 환경의 가변성을 해결하여 사운드가 장애물 위로 전달되어 최적의 청취자 경험을 제공하고 360°의 지향각을 가져야 한다. 변압기 탭으로 로우와 하이 임피던스에서 모두 사용 가능 하여야 한다.

(2) 기기특성

[ System Details ]

- Effective frequency range	: 55 Hz - 25 kHz

- Rated noise power	: 80 W

- Broadband sensitivity	: >84 dB @1 W/1M (200 - 10 kHz)

- Coverage angle (-6 dB)	: 360° (500 Hz – 5 kHz)

- Maximum continuous SPL	: 104 dB

- Maximum peak SPL	: 110 dB

- Rated impedance	: 16 Ω

- Transformer taps	: 7.5 W, 15 W, 30 W, 60 W /

15 W, 30 W, 60 W

- Transducer	: (1)  5.25 in (135 mm) weather

resistant cone woofer, ferrite magnet,

rubber surround

(1)  2x1 in (25mm) aluminum

dome tweeter, rubber surround

- Input connector type	: Wire pig-tail, blunt

- Enclosure material	: Glass-Filled polypropylene,

F1-F2 UL Rated

- Grille material	: Polyester fabric on polycarbonate

frame

- Mount	: Direct to concrete

[ ENCLOSURE DETAILS ]

- Ingress protection	: IP - 55

- Operating environment	: Designed for outdoor use

- Product dimensions (HWD)	: 30.16 in (766mm) x 6.46 in (164mm)

x 6.46 in (164mm)

(not including base support)

- Net Weight	: 10.36 lb (4.7 kg)

** AD-DWL.360 또는 동등 이상품 이어야 한다.