LINE ARRAY SPEAKER

━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━

(1) 기능

본 기기는 저음 반사형 인클로저에 8인치 트랜스듀서와 고주파 압축 드라이버를 탑재하여 소규모 스포츠 경기장부터 강당이나 강의실에 이르기까지 광범위한 애플리케이션에 프리미엄 사운드를 제공할 수 있어야 한다. Q-SYS 네트워크 앰프와 페어링하면 맞춤형 라우드 스피커 보이싱과 보호 기능부터 고급 원격 측정까지 여러 가지 이점이 확장되어 배포 속도를 높이고 최적의 시스템 운영 환경을 제공할 수 있어야 한다. 실내 및 보호된 실외 환경을 위한 방수(IP54) ABS 인클로저를 사용하고 최대 12개의 스피커를 리깅 할 수 있어야 한다.

(2) 기기특성

- Enclosure configuration	: Bass Reflex, two-way passive/bi-amp

line array loudspeaker

- Coverage (horizontal x vertical)	: 100° x 15°

- System bandwidth (-10dB with EQ)	: -10 dB: 60 Hz - 20 kHz

- Crossover HF-LF	: 1.6 kHz (passive) / 1.5 kHz (bi-amp)

- Sensitivity	: 101.5 dB

- LF sensitivity	: 91 dB

- HF sensitivity	: 109 dB

- Max SPL (continuous)	: 116 dB (passive) / 120 dB (bi-amp)

- Max SPL (peak)	: 128 dB (passive) / 132 dB (bi-amp)

- Power rating	: 46 Vrms,

continuous power 260W @ 8 Ω,

rated power 520 W @ 8 Ω

- LF power rating	: 45 Vrms,

continuous power 250 W @ 8 Ω,

rated power 500 W @ 8 Ω

- HF power rating	: 31 Vrms,

continuous power 60 W @ 16 Ω,

rated power 120 W @ 16 Ω

- Nominal impedance	: 8 Ω (passive), 8 Ω (LF), 16 Ω (HF)

- Weatherization	: IP54; Stainless screws;

UV and Corrosion treated grille;

Aluminum Rigging

Hydrophobic Stainless SteelMesh

behind grille; Input cup (IP65)

sealing with gland

- Dimensions (HxWxD)	: 272 x 512 x 349 mm

- Weight	: 12.4 kg

** PL-LA8 또는 동등 이상품 이어야 한다.