DIGITAL SIGNAL PROCESSOR

━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━

(1) 기능

본 기기는 Linux 운영 체제를 실행하는 Intel 프로세서를 사용하여 모든 실시간 오디오, 비디오 및 제어 처리를 수행하는 프로세서로 표준 기가비트 이더넷 인프라에서 기본적으로 작동하여야 한다. 최대 160 x 160 네트워크 오디오 채널을 제공하며, Q-LAN, AES67 또는 Dante 포맷 네트워크 오디오로 개별적으로 구성할 수 있어야 한다. 8 x 8 소프트웨어 기반 Dante 네트워크 오디오 채널을 포함하며, 최대 64 x 64 소프트웨어 기반 Dante 용량에 대한 라이선스를 제공할 수 있어야 한다. 총 24개의 아날로그 I/O 용량을 지원하며, 8개의 마이크/라인 입력, 8개의 라인 출력, 8개의 플렉스 채널 I/O로 구성되며, 최대 8개의 VoIP 인스턴스, 24x AEC 프로세서로 시스템에 맞는 통합된 오디오/비디오 제어 솔루션을 제공할 수 있어야 한다. 오디오와 비디오, 컨트롤까지 할 수 있는 통합 시스템 Q-SYS 소프트웨어로 프로그램을 디자인하고, 사용자 맞춤 UCI로 Touch Screen 외에도 iPad, iPhone로 원격제어가 가능하여야 한다. Dante, AES67의 다양한 형식의 네트워크 오디오와 RS-232/GPIO 포트를 가지는 외부기기와 연동 및 제어가 가능하고, 기업, 고등 교육, 엔터테인먼트 및 접객 등 다양한 분야에서  맞춤형 시스템을 구축할 수 있어야 한다.

(2) 기기특성

[ Processing ]

- Processor	: Intel 64-bit architecture

- Audio processing	: 32-bit floating point

- Q-LAN network audio transport	: 32-bit floating point

[ Q-SYS Capacities ]

- Network audio I/O	: 160 x 160

- Analog I/O	: 24x

(8x mic/line in, 8x line out, 8x flex)

- Dante channels	: 8 x 8 included (up to 64 x 64 with	Software-based Dante feature license)

- AEC channels	: 24

- Q-SYS NM-T1 capacity	: 8

- WAN / media streaming channels	: 36 x 36

- Network peripherals	: Up to 96

- VoIP softphones	: 8

- Audio recording / playback	: 4 channels recording / 16 channels	playback, [expandable up to 64	channels playback with optional multi	track playback license (SLMTP-32)	stackable up to 2x]

- Media drive capacity	: 128 GB (at least 100 GB available	for user media, or at least 200 hours	of uncompressed 48kHz, 24 bit,	mono WAV format audio files)

[ Control ]

- RS232	: 2 ports

- GPIO	: 8 x 8

[ USB Inputs & Outputs ]

- USB	: 2x USB-A and 1x USB-C port

- AV bridging	: Via USB-C

- USB HID routing	: Via USB-C

- USB audio device hosting	: Support for standard USB headset,	speakerphone on USB-C connection	(3 devices max at a time, each	having up to 8x8 USB audio	channels, up to 16x16 total channels)

USB-C (Audio bridging)

- Bit depth	: 24 bit

- Channel count	: 16 x 16

- Sample rate	: 48 kHz

USB-A Input

- Sample rate	: 48 kHz or 16 kHz, mono

- Resolution	: 8-bit, 16-bit, 24-bit or 32-bit, float

- Format	: Little-endian, signed or unsigned

USB-A Output

- Sample rate	: 48 kHz only, stereo

- Resolution	: 8-bit, 16-bit, 24-bit or 32-bit, float

- Format	: Little-endian, signed or unsigned

[ Physical ]

- Product Dimensions (WDH)	: 19.0 x 12.2 x 1.7 in

(482.6 x 310.9 x 43.6 mm)

- Power Consumption	: 60 W typical, 150 W maximum

- Net Weight	: 12.0 lb (5.44 kg)

** CORE 24f 또는 동등 이상품 이어야 한다.