DIGITAL SIGNAL PROCESSOR

━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━

(1) 기능

본 기기는 중앙 집중식 또는 엣지 처리 배포 아키텍처 설계에 사용하도록 설계된 완전히 통합된 오디오, 비디오 및 제어 프로세서로 Q-SYS 풀 스택 AV 플랫폼과 엔터프라이즈급 서버 하드웨어를 결합하여 중대형 애플리케이션을 위한 유연하고 확장 가능한 오디오, 비디오 및 제어 솔루션을 제공할 수 있어야 한다. 최소 256 x 256 채널의 네트워크 채널 용량을 제공하며, 각 스트림은 기본 Q-LAN 네트워크 오디오 형식 또는 AES67 형식 오디오 스트림으로 구성 가능하고, 최대 64 x 64 채널의 일반 미디어/WAN 스트리밍 용량도 지원할 수 있어야 한다. 8 x 8 소프트웨어 기반 Dante 네트워크 오디오 채널을 포함하며, 최대 128 x 128 소프트웨어 기반 Dante 용량에 대한 라이선스를 제공할 수 있어야 한다. 최대 4트랙의 오디오 녹음과 16트랙의 오디오 재생을 지원하며, 오디오 재생 용량은 소프트웨어 라이선스를 통해 최대 128트랙까지 확장할 수 있어야 한다. 최대 32개의 VoIP 인스턴스, 64x AEC 프로세서로 시스템에 맞는 통합된 오디오/비디오 제어 솔루션을 제공할 수 있어야 한다. 오디오와 비디오, 컨트롤까지 할 수 있는 통합 시스템 Q-SYS 소프트웨어로 프로그램을 디자인하고, 사용자 맞춤 UCI로 Touch Screen 외에도 iPad, iPhone로 원격제어가 가능하여야 한다. 분산 네트워크 I/O를 사용하거나 분산 처리 시스템과 함께 사용하여 여러 구역 또는 공간을 위한 중앙 프로세서로 효과적으로 작동하여 다양한 분야에서  맞춤형 시스템을 구축할 수 있어야 한다.

(2) 기기특성

[ Q-SYS Capacities ]

- Network audio I/O	: 256 x 256

- Dante network I/O	: 8 x 8 included (up to 128x128 with	Software-based Dante feature license)

- Media/WAN channel capacity	: 64 x 64

- VoIP softphones	: 32

- AEC channels	: 64

- Audio recording / playback	: 4 channels recording / 16 channels	playback, [expandable up to 128	channels playback with optional multi	track playback license (SLMTP-32)	stackable up to 4x]

- Media drive capacity	: 256 GB (at least 200 GB available	for user media, or at least 400 hours	of uncompressed 48kHz, 24 bit,	mono WAV format audio files)

[ Hardware ]

- Power	: 1x universal input,

500W PSU module

- LAN	: 4x 2500 Mbps ports

(2x Q-SYS Multimedia, 2x Q-SYS Aux)

- RS232	: 1x DB-9 RS-232 port (rear panel),	16550-compliant

- USB	: 2 USB-A and 2 USB-C port

- Ventilation	: Forced air – front intake,

rear exhaust

[ Controls and Indicators ]

- Front	: Power LED

Front Panel LCD module,

white backlight

4 navigation buttons

(up, down, left, right) +

1 selection button to navigate	between screens on the front display

[ Packaging and Accessories ]

- Product Dimensions (WDH)	: 18.11 x 17.24 x 1.73 in

(460 x 438 x 44 mm)

- Net Weight	: 18.7 lb (8.5 kg)

** Server Core X10 또는 동등 이상품 이어야 한다.