DIGITAL SIGNAL PROCESSOR

━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━

(1) 기능

본 기기는 중앙 집중식 또는 엣지 처리 배포 아키텍처 설계에 사용하도록 설계된 완전히 통합된 오디오, 비디오 및 제어 프로세서로 Q-SYS 풀 스택 AV 플랫폼과 엔터프라이즈급 Dell 서버 하드웨어를 결합하여 대규모 애플리케이션을 위한 유연하고 확장 가능한 오디오, 비디오 및 제어 솔루션을 제공할 수 있어야 한다. 최소 384 x 384 채널의 네트워크 채널 용량을 제공하며, 각 스트림은 기본 Q-LAN 네트워크 오디오 형식 또는 AES67 형식 오디오 스트림으로 구성 가능하고, 최대 96 x 96 채널의 일반 미디어/WAN 스트리밍 용량도 지원할 수 있어야 한다. 8 x 8 소프트웨어 기반 Dante 네트워크 오디오 채널을 포함하며, 최대 256 x 256 소프트웨어 기반 Dante 용량에 대한 라이선스를 제공할 수 있어야 한다. 최대 4트랙의 오디오 녹음과 16트랙의 오디오 재생을 지원하며, 오디오 재생 용량은 소프트웨어 라이선스를 통해 최대 256트랙까지 확장할 수 있어야 한다. 최대 64개의 VoIP 인스턴스, 128x AEC 프로세서로 시스템에 맞는 통합된 오디오/비디오 제어 솔루션을 제공할 수 있어야 한다. 오디오와 비디오, 컨트롤까지 할 수 있는 통합 시스템 Q-SYS 소프트웨어로 프로그램을 디자인하고, 사용자 맞춤 UCI로 Touch Screen 외에도 iPad, iPhone로 원격제어가 가능하여야 한다. 중앙 프로세서 역할을 수행하고 네트워크 I/O를 가장 필요한 곳으로 효율적으로 분배하여 향상된 처리 성능과 네트워크 채널 용량이 필요한 애플리케이션을 지원하여 다양한 분야에서 맞춤형 시스템을 구축할 수 있어야 한다.

(2) 기기특성

[ Q-SYS Capacities ]

- Network audio I/O	: 384 x 384

- Dante network I/O	: 8 x 8 included (up to 256x256 with	Software-based Dante feature license)

- Media/WAN channel capacity	: 96 x 96

- VoIP softphones	: 64

- AEC channels	: 128

- Audio recording / playback	: 4 channels recording / 16 channels	playback, [expandable up to 128	channels playback with optional multi	track playback license (SLMTP-32)	stackable up to 8x]

- Media drive capacity	: 480 GB (at least 400 GB available	for user media, or at least 800 hours	of uncompressed 48kHz, 24 bit,	mono WAV format audio files)

[ Hardware ]

- Platform	: Dell R360XE

- Power	: 2x universal input,

600W PSU module

- LAN	: 4x 1000 Mbps ports

(2x Q-SYS Multimedia, 2x Q-SYS Aux)

- RS232	: 1x DB-9 RS-232 port (rear panel),	16550-compliant

- USB	: 2 USB-A

- VGA	: 1x VGA port

- iDRAC	: 1x dedicated iDRAC v9 Ethernet port

1x iDRAC Direct (Micro-AB USB) port

- Ventilation	: Forced air – front intake,

rear exhaust

[ Controls and Indicators ]

- Front	: Blue Power LED

White LED

Device Rest Button

Front Panel LCD module displays IP	address

2 navigation buttons

(left, right) +

1 selection button to navigate	between screens on the front display

[ Packaging and Accessories ]

- Product Dimensions (WDH)	: 23.6 x 19.0 x 1.68 in

(599 x 482.0 x 42.8 mm)

- Net Weight	: 29.17 lb (13.23 kg)

** Server Core X20r 또는 동등 이상품 이어야 한다.