NETWORK MULTI-PURPOSE I/O EXPANDER

━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━

(1) 기능

본 기기는 네트워크 오디오 및 제어 연결 확장기로 Q-SYS 시스템의 기능을 확장하여 네트워크에 연결되지 않은 오디오 및 제어 장치와의 원활한 상호 운용성을 지원할 수 있어야 한다. 처리 하드웨어에서 로컬 I/O를 분리함으로써 원하는 토폴로지를 지원하기 위해 쉽게 확장이 가능한 모듈형 네트워크 I/O 제품이어야 한다. 4개의 소프트웨어 구성 가능한 Flex 오디오 I/O 채널, 타사 제어 주변 장치와의 통합을 위한 4x8 GPIO 및 1개 RS232 직렬 포트, 스피커를 위한 2개의 앰프 출력이 있어야 한다. PoE(Power over Ethernet)를 지원하고 단일 네트워크 실행에서 최대 4개의 확장기를 데이지 체인 방식으로 연결하여 더 적은 수의 네트워크 포트를 사용할 수 있어야 한다. 표면 또는 하프 랙 너비의 1U 사이즈 랙 장착이 가능하여야 한다.

(2) 기기특성

- Connectivity	: TFour (4) Flex I/O, 4x8 GPIO, one (1)	RS232, two (2) amplifier outputs

Mic/Line Inputs

- Maximum input level	: +24 dBu (balanced),

+18 dBu (unbalanced)

- Preamplifier gain range	: 0 dB to 60 dB

- Phantom power	: +48 V DC (10 mA per channel,

IEC 61938 P48 compliant)

- Equivalent input noise	: <-120 dBu, no weighting

@ 20 Hz to 20 kHz

- Input to input crosstalk @ 1 kHz	: > 110 dB Typical, > 95 dB Minimum

- Input impedance	: 10 kΩ (balanced), 5 kΩ (unbalanced)

- Input Dynamic Range	: @ +24 dBu sensitivity, > 108 dB

@ +10 dBu sensitivity, > 105 dB

@ -10 dBu sensitivity,  > 100 dB

@ -36 dBu sensitivity,  > 80 dB

Mic/Line Outputs

- Max output level range	: -37 dBu to +24 dBu

- Output dynamic range	: 108 dB

- Output to output crosstalk @ 1 kHz	: > 102 dB Typical, > 90 dB Minimum

- Output impedance	: 200 Ω (balanced),

100 Ω (unbalanced)

- Sample rate	: 48 kHz

- Bit depth	: 24 bit

Amp Outputs

- Max speaker output power (Aux 24VDC Power)	: 9 W @ 4 Ω, per channel

- Max speaker output power (PoE+)	: 5 W @ 4 Ω, per channel

- Output impedance	: 4-8 Ω nominal

Control

- RS232	: 1 port

- GPIO	: 4x8

Other Connectors

- External power supply	: 24 VDC nominal, 3.7 A on Euro	connector with second connector for	daisy-chaining (QIO-PSU power	supply sold separately)

- LAN (PoE)	: Gigabit LAN connection for Q-LAN,

PoE

- PoE specification	: Conforms to IEEE 802.3at Type 2,	Class 4

Accepts IEEE 802.3af Type 1, Class 3	(amplifier disabled at this power level)

- LAN (Thru)	: Ethernet daisy-chaining

General

- Dimensions ( D x W x H )	: 5.5 x 8.62 x 1.59 in

(139.7 x 219.1 x 40.4 mm)

- Weight	: 2.3 lbs. (1.04 kg)

** QIO-FLEX4A 또는 동등 이상품 이어야 한다.