NETWORK DIGITAL AUDIO I/O EXPANDER

━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━

(1) 기능

본 기기는 네트워크 디지털 오디오 I/O 확장기로 AES3 연결을 통해 네트워크에 연결되지 않은 디지털 오디오 장치와의 상호 운용성을 지원할 수 있어야 한다. 처리 하드웨어에서 로컬 I/O를 분리함으로써 원하는 토폴로지를 지원하기 위해 쉽게 확장이 가능한 모듈형 네트워크 I/O 제품이어야 한다. AES3의 총 8개의 입력 및 출력 채널을 가지며, PoE(Power over Ethernet)를 지원하고 단일 네트워크 실행에서 최대 4개의 확장기를 데이지 체인 방식으로 연결하여 더 적은 수의 네트워크 포트를 사용할 수 있어야 한다. 표면 또는 1/4 너비의 1U 사이즈 랙 장착이 가능하여야 한다.

(2) 기기특성

Connectivity	: Four (4) stereo pairs of AES3 digital	inputs and four (4) stereo pairs of	AES3 digital outputs

(8 input and output channels total)

AES3 Digital I/O

- Input impedance	: 110 Ω (balanced)

- Output impedance	: 110 Ω (balanced)

- Group delay	: 65 samples with SRC enabled

- Sample rate	: 44.1 kHz, 48 kHz, 88.2 kHz, 96 kHz,	176.4 kHz, 192 kHz

(with sample rate conversion to	Q-SYS system rate of 48 kHz)

- Bit Depth	: 24 bit

Other Connectors

- External power supply	: 24 VDC nominal, 2.5 A on Euro

connector with second connector for

daisy-chaining (QIO-PSU power

supply sold separately)

- LAN (PoE)	: Gigabit LAN connection for Q-LAN,

PoE

- PoE specification	: Conforms to IEEE 802.3af Type 1,	Class 2

- LAN (Thru)	: Ethernet daisy-chaining

General

- Dimensions ( D x W x H )	: 8.5 x 4.25 x 1.59 in

(215.9 x 108 x 40.4 mm)

- Weight	: 1.72 lb (0.78 kg)

** QIO-AES8x8 또는 동등 이상품 이어야 한다.