NETWORK ANALOG TELEPHONY I/O EXPANDER

━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━

(1) 기능

본 기기는 아날로그 전화 연결 확장기로 Q-SYS 시스템의 기능을 확장하여 아날로그 전화 시스템과의 효율적인 상호 운용성을 지원할 수 있어야 한다. 처리 하드웨어에서 로컬 I/O를 분리함으로써 원하는 토폴로지를 지원하기 위해 쉽게 확장이 가능한 모듈형 네트워크 I/O 제품이어야 한다. 표준 RJ-11 커넥터에 두개의 POTS 전화선이 있어야 한다. PoE(Power over Ethernet)를 지원하고 단일 네트워크 실행에서 최대 4개의 확장기를 데이지 체인 방식으로 연결하여 더 적은 수의 네트워크 포트를 사용할 수 있어야 한다. 표면 또는 1/4 너비의 1U 사이즈 랙 장착이 가능하여야 한다.

(2) 기기특성

- Connectivity	: Two (2) PSTN (POTS) phone lines on	standard RJ11 (6P2C) connectors

Telephone Lines

- Impedance	: 600 Ω, nominal

- Frequency response	: 300 Hz to 3.3 kHz, ±1.0 dB

- THD+Noise	: < 0.5%

- Signal-to-noise ratio	: > 62 dB

- Ringer Equivalence Number	: 0.1

Other Connectors

- External power supply	: 24 VDC nominal, 2.5 A on Euro

connector with second connector for

daisy-chaining (QIO-PSU power

supply sold separately)

- LAN (PoE)	: Gigabit LAN connection for Q-LAN,

PoE

- PoE specification	: Conforms to IEEE 802.3af Type 1,	Class 1

- LAN (Thru)	: Ethernet daisy-chaining

General

- Dimensions ( D x W x H )	: 8.5 x 4.25 x 1.59 in

(215.9 x 108 x 40.4 mm)

- Weight	: 1.63 lb (0.74 kg)

** QIO-TEL2 또는 동등 이상품 이어야 한다.