CEILING SPEAKER

━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━

(1) 기능

본 기기는 6.5인치 2-way 천정형 스피커로 제로 베젤 디자인을 가지고 있어야 한다. 70/100V 멀티탭 트랜스포머가 장착되어 있으며, 바이패스를 통해 16옴 스피커 시스템과 함께 사용할 수 있어야 한다. 스냅핏 자석 그릴을 가지며, 흠집 없는 제거 가능한 로고를 가지고 있어야 한다. Q-SYS를 통해 Advanced Intrinsic Correction 보이싱 기술을 사용할 수 있어야 한다.

(2) 기기특성

- Effective frequency range	: 65 Hz – 20 kHz

- Rated noise power / voltage	: 60 watts / 31 volts (rms)

- Sensitivity	: 88 dB

- Rated coverage (-6 dB)	: 135° conical DMT™

- Directivity factor (Q)	: 6.5

- Directivity index (DI)	: 8 dB

- Maximum continuous SPL	: 106 dB

- Maximum peak SPL	: 112 dB

- Nominal impedance	: 16 Ω

- Recommended amplifier	: 60 watts

- Transformer taps / impedance	: 16Ω (in bypass setting)

7.5W (70V); 15W (100V) Tap: 667Ω

15W (70V); 30W (100V) Tap: 333Ω

30W (70V); 60W (100V) Tap: 167Ω

60W (70V); N/A (100V) Tap: 83Ω

- LF transducer	: 165 mm [6.5-inch] weather resistant	paper cone woofer

- HF transducer	: 19 mm [0.75-inch] aluminum dome	tweeter

- Input connector type	: Euroblock connector with parallel	output

- Enclosure material	: ABS baffle on powder coated steel	back can

- Grille material	: Powder coated steel

Ingress protection	: IP-34

Cutout dimension	: Ø 245 mm [Ø 9.65-inch]

Net weight	: 4.3 kg [9.5 lb]

Product dimensions (Diameter x Height)	: Ø 280 x 237 mm

[Ø 11.02 x 9.32-inch]

** AD-C6T-ZB 또는 동등 이상품 이어야 한다.