CEILING SPEAKER

━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━

(1) 기능

본 기기는 10인치 2-way 천정형 스피커로 제로 베젤 디자인을 가지고 있어야 한다. 70/100V 멀티탭 변압기가 장착되어 있으며, 바이패스를 통해 8옴 스피커 시스템과 함께 사용할 수 있어야 한다. 스냅핏 자석 그릴을 가지며, 흠집 없는 제거 가능한 로고를 가지고 있어야 한다. Q-SYS를 통해 Advanced Intrinsic Correction 보이싱 기술을 사용할 수 있어야 한다.

(2) 기기특성

- LF transducer	: 10 in (254 mm), 2.0 in. (50.8 mm)	voice coil, ferrite

- HF transducer	: Coaxial compression driver,

1.5 in (38.1 mm) voice coil

- Enclosure configuration	: Two-way, ceiling loudspeaker,

Sealed

- System bandwidth	: -3 dB: 86 Hz - 20 kHz

-6dB: 76 Hz-20 kHz

-10 dB: 68 Hz-20 kHz

- Sensitivity	: 92.5 dB @ 1 W/1 m

- Coverage	: 90° conical DMT

- Max SPL (continuous)	: 116 dB

- Max SPL (peak)	: 128 dB

- Max SPL (calculated)	: 122 dB

- Power rating	: Continuous power 250 W @ 8Ω,	rated Power 500 W

- Bypass impedance	: 8 Ω

- Minimum impedance	: 6.9 Ω @ 20 hz

- Transformer taps (70v/100v)	: 25 W, 50 W, 100 W, 200 W /

50 W, 100 W, 200 W

- Enclosure material	: ABS baffle on powder coated steel	back can

- Connectors	: 4-pin 0.2 in (5 mm) Euroblock	connector with parallel output

Ingress protection	: IP-44

Cutout dimension	: 305 mm

Net weight	: 10.5 kg [23 lb]

Dimensions (H x W x D)	: 342.9 x 342.9 x 349.25 mm

[13.5 x 13.5 x 13.75 in]

** AD-C10T-HPZB 또는 동등 이상품 이어야 한다.