DIGITAL AUDIO MIXER

━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━

(1) 기능

본 기기는 디지털 오디오 믹서로서, 12채널의 XLR 입력과 4채널의 콤보(XLR/TRS)입력, 2채널의 스테레오 TRS 입력 및 USB를 통한 Stereo(.mp3) Playback 이 가능하여야 한다.  Main L/R 출력(XLR), 6채널 Aux 출력(XLR) + 2개의 스테레오 인이어 모니터 or 모노 벨런스 Aux 출력(1/4“ TRS) 이 가능하여야 한다. Cue 및 Monitor L/R 은 각각 1개이며 1/4” Stereo, TRS 출력 이 가능하여야 한다. 8개의 DCA 그룹과 뮤트 그룹을 지원하여야 한다. 터치스크린을 이용한 직관적이고 간편한 컨트롤과 조그셔틀을 이용한 세밀한 컨트롤이 가능하여야 한다. 모든 프로세싱은 Simple mode와 Advanced mode 두 가지로 컨트롤이 가능하여야 하며, 모든 출력채널에는 프로세서(Graphic equalizer, Limit, Time delay, Powered speaker preset data)가 내장되어 있어야 한다.

기본 제공되는 Wi-Fi dongle을 이용하여 지정된 iOS 또는 Android 장치의 어플을 통한 원격제어 및 무선 멀티스크린 오퍼레이팅이 가능하여야 하며, USB를 통한 플레이 및 하드 레코딩과 믹서 프리셋 데이타를 복사할 수 있어야 한다. Wizard 기능은 FX와 Gain을 저장된 데이터를 이용하여 일괄 손쉽게 설정할 수 있어야 한다.

(2) 기기특성

- Display	: 7"(178mm) diagonal color TFT,

capacitive touch sensing

[Inputs]

- Total	: 22

- Mic/Line	: 16(12 XLR, 4 XLR combo)

- Line	: 2 Stereo, 1/4" TRS

- Stereo USB	: Stereo USB/MP3 playback

- Talkback	: 1(XLR)

[Input channel processing]

- EQ	: 4-band parametric EQ with Hi/Low

Shelving option, Variable

24dB/octave HPF and LPF

Dynamics	: Gate, Compressor

Delay	: Delay(100 msec max)

[Output]

Total	: 12

Main L/R	: 2 (XLR Line-level)

Aux	: 6 (XLR, line-level) +2(TRS,stereo In-Ear Monitor
or mono balanced line-level)
* inEar Monitor (Stereo)	: 2 (TRS, 16ohm min. impedance.
from Auxes7/8 and 9/10)

Que	: 1 (Stereo, TRS, Line or headphone,
16ohm min. impedance)

Monitor L/R	: 1 (Stereo, TRS, Line or headphone,
16ohm min. impedance)

[Output channel processing]

- EQ	: 1/3 octave graphic EQ(main L/R,

auxes 1-6), 6-band parametric EQ,

variable HPF and LPF

- Anti-feedback filters	: 8-band anti-feedback filters

- Dynamics	: Limiter

- Delay	: 100msec

[Recording/Playback]

- Multi-track	: 22 x 22 tracks direct to hard drive

- MP3	: Stereo USB/MP3 playback

[Groups]

- DCA	: 8(with Mutes)

- Mute	: 8

- Cue	: Selectable. AFL, PFL

[Effects]	: 4 simultaneous, professional effects

engines including reverb, echo,

delay, chorus, pitch shift

- 1 pitch correct (assignable to any mono input channel)
: 1 pitch correct(assignable to any mono
input channel)

- Real time analyzer(RTA)	: 1(1/3 octave. Assignable to

channels or user selectable source)

- Preset memory	: 99 user scenes, 120 factory

presets, 99 user presets

- Digital connections	: 2 USB A connectors

- External control	: TouchMix-8/16 control app for

iOS® and Android™ devices

controls all mixer functions via

Wi-Fi

- WiFi	: USB Wi-Fi adaptor(included) or

external Wi-Fi router(requires USB

to ethernet adaptor)

[Dimensions(HWD)]

- Shipping	: 4.75in x 24.5in x 15in

(12cm x 62cm x 38.1cm)

- Mixer only	: 2.3in x 14.2in x 11.5in

(5.8cm x 36cm x 29.1cm)

[Weight]

- Shipping	: 11lb(4.9kg)

- Mixer only	: 5.9lb(2.98kg)

- Power requirements	: 42W, 100~240 VAC, 50~60 Hz

- Sampling frequency	: Selectable 44.1kHz or 48kHz

- Internal processing	: 32-bit floating point

- THD	: <0.005%, +4dBu; 20Hz~20kHz, unity

gain, any input to any output

- Frequency response	: 20Hz~20kHz +/-0.5dB, any input to

any output

- Dynamic range	: 105dB

- Equivalent input noise	: -126dBu

- Residual output noise	: -86dBu

- Crosstalk	: -80dB

- S/N ratio	: -94dB

- Gain(mic inputs)	: 75dB(60dB analog, 15dB digital)

- Maximum input level	: +16dBu(mic/line inputs, XLR),

+26dBu(mic/line inputs, TRS),

+22dBu(stereo inputs)

- Maximum output level	: +22dBu(all line-level outputs)

- Phantom power	: 48V, all mic inputs, individually

switchable

** TouchMix-16 또는 동등 이상품 이어야 한다.