DIGITAL MIXING CONSOLE

━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━

(1) 기능

본 기기는 디지털 믹싱 콘솔로서, 24채널의 모노입력과 6채널의 스테레오 입력을 지원하며, 2채널의 메인 출력과 14채널의 Aux 출력 및 8개의 DCA 그룹과 뮤트 그룹을 지원하여야 한다. 터치스크린을 이용한 직관적이고 간편한 컨트롤과 조그셔틀을 이용한 세밀한 컨트롤이 가능하여야 한다. 모든 출력채널에는 프로세서(Graphic equalizer, Limit, Comp, Time delay, Powered speaker preset data)가 내장되어 있어야 한다.

무선휴대기기 어플을 통한 원격제어 및 무선 멀티스크린 오퍼레이팅이 가능하여야 하며, USB를 통한 플레이 및 하드 레코딩과 믹서 프리셋 데이타를 복사할 수 있어야 한다. Wizard 기능은 FX와 Gain을 저장된 데이터를 이용하여 일괄 손쉽게 설정할 수 있어야 한다.

(2) 기기특성

- Display	: 10"(254mm) diagonal,

1024 x 600 pixel, color TFT,

capacitive multi-touch sensing

[Inputs]

- Total	: 32

- Mic/Line	: 24(20 XLR, 4 XLR combo)

- Line	: 6(balanced, 1/4" TRS+top panel

1/8"(3.5mm) stereo)

- Stereo USB	: Stereo USB/MP3 playback

- Talkback	: 1(XLR, 48V)

[Input channel processing]

- EQ	: 4-band parametric EQ with Hi/Low

shelving option, variable

24dB/octave HPF and LPF

- Dynamics	: Gate, compressor

- Delay	: Delay(100msec max)

- Automatic microphone mixer	: Gain sharing, 24 channels, 2 auto

mixers(requires firmware version

1.3 or higher)

[Outputs]

- Total	: 16

- Main L/R	: 14(XLR line-level)

- Aux	: 6(XLR, line-level)+2(TRS, stereo

In-ear monitor or mono balanced

line-level)

- In ear monitor(stereo)	: 2(TRS, 16ohm min. impedance,

from Auxes 11/12 and 13/14)

- Cue	: 2(stereo, TRS, line or headphone,

16ohm min. impedance)

- Monitor L/R	: 1(stereo TRS, line or headphone,

16ohm min. impedance)

[Output channel processing]

- EQ	: 1/3 octave graphic EQ(main L/R,

auxes 1-6), 6-band parametric EQ,

variable high- and low-pass

filters

- Anti-feedback filters	: 12-band anti-feedback filters

- Dynamics	: Compressor/limiter

- Delay	: 100msec

[Recording/Playback]

- Multi-track	: 32 x 32 tracks direct to hard drive

- DAW	: 32 x 32 tracks (Mac OS® and

Windows®)

- MP3	: Stereo USB/MP3 playback

[Groups]

- DCA	: 8(with mutes)

- Mute	: 8

- Sub groups	: 8(with 6-band parametric EQ, HPF

and LPF, limiter)

- Cue	: Selectable. AFL, PFL, solo in place

[Effects]	: 6 simultaneous, professional effects

engines including reverb, echo,

delay, chorus, pitch shift

4 simultaneous

- 1 pitch correct

(assignable to any mono input channel)	: 1 pitch correct(assignable to any

mono input channel)

- Real time analyzer(RTA)	: 2(1/3 octave, assignable to

channels or user selectable source)

- Preset memory	: 99 user scenes, 120 factory

presets, 99 user presets

- Digital connections	: 2 USB A connectors,

1 USB B connector,

1 RJ-45 port(connection for Wi-Fi

router)

- External control	: TouchMix-30 control app for iOS®

and Android™ devices controls all

mixer functions via Wi-Fi.

- WiFi	: Requires external ethernet Wi-Fi

router(recommended) or USB

Wi-Fi adaptor(not included)

[Dimensions(HWD)]

- Shipping	: 12in X 23.7in X 19.5in

(30.5cm X 60.3cm X 49.5cm)

- Mixer only	: 7.5in X 16.9in X 18.1in

(19cm X 42.9cm X 46cm)

[Weight]

- Shipping	: 25.2lb(11.4kg)

- Mixer only	: 17.5lb(7.9kg)

- Power requirements	: 85W, 100~240 VAC, 50~60 Hz

- Sampling frequency	: Selectable 44.1kHz or 48kHz

- Internal processing	: 32-bit floating point

- THD	: <0.005%, +4dBu; 20Hz~20kHz, unity

gain, any input to any output

- Frequency response	: 20Hz~20kHz +/-0.5dB, any input to

any output

- Dynamic range	: 105dB

- Equivalent input noise	: -126dBu

- Residual output noise	: -86dBu

- Crosstalk	: -80dB

- S/N ratio	: -94dB

- Gain(mic inputs)	: 75dB(60dB analog, 15dB digital)

- Maximum input level	: +16dB(XLR mic/line inputs),

+26dB(TRS mic/line inputs),

+24dBu(TRS line inputs),

0dBv(top panel 1/8" stereo input)

- Maximum output level	: +22dBu(all line-level outputs)

- Phantom power	: 48V, all mic inputs, individually

switchable

** TouchMix-30 Pro 또는 동등 이상품 이어야 한다.