CEILING SPEAKER

━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━

(1) 기능

본 기기는 8인치 2웨이 천장형 스피커로 8인치 우퍼에는 다습한 환경에 강한 폴리프로필렌 콘이 장착되어 있고 밀폐형 인클로져는 52Hz 이하의 저주파를 전달하는 데에 최적화되어 있어야 하며 우퍼와 선대칭으로 장착된 기존의 트위터 타입에서 자주 발생하던 간섭 현상을 줄이기 위해, 트위터는 우퍼의 중심부에서 약간 빗겨 장착이 되어 있어야 한다. 하이임피던스 용 트랜스포머가 장착되어 8옴 뿐 아니라 70V 및 100V로 변환하여 전관방송에도 적합한 기기이어야 한다.

(2) 기기특성

- Effective frequency range	: 52Hz~20kHz

- Rated noise power/voltage	: 80W/25.3V (rms)

- System sensitivity	: 89dB SPL

- Coverage angle(-6dB)	: 100˚(500Hz~5kHz)

- Maximum continuous SPL	: 108dB

- Maximum peak SPL	: 114dB

- Rated bypass impedance	: 8ohms

- Transformer taps

70V	: 60, 30, 15, 7.5, 3.8 watts

100V	: 60, 30, 15, 7.5 watts

8ohm bypass

- HF transducer	: 22mm[.86in] silk dome tweeter,

coaxially mounted

- LF transducer	: 210mm[8in] polypropylene cone

with butyl rubber surround

- Input connector type	: Euroblock connector with parallel

output terminals

- Baffle material	: Painted ABS polymer

- Grille material	: Painted steel

- Back can material	: Plated steel

- Testing	: Listed UL1480, UL2043 safe for use

in air handling space

- Net weight	: 5.2kg[11.5lb]

- Product dimensions	: Φ316 x 288 mm

[Φ12.4 x 11.3 in]

- Cut-Out dimensions	: 285mm[11.2in]

- Ceiling capture thickness	: 6~38 mm

[0.25~1.5 in]

- Shipping weight	: 13.3kg[29.3lb] (pair packed)

- Shipping dimensions	: 743 x 381 x 381 mm

[29.3 x 15 x 15 in]

** AC-C8T 또는 동등 이상품 이어야 한다.