SPEAKER

━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━

(1) 기능

본 기기는 4인치 2웨이 스피커로 4인치 우퍼에는 다습한 환경에 강한 폴리프로필렌 콘이 장착되어 있고 밀폐형 인클로져는 70Hz 이하의 저주파를 전달하는 데에 최적화되어 있어야 하며 우퍼와 선대칭으로 장착된 기존의 트위터 타입에서 자주 발생하던 간섭 현상을 줄이기 위해, 트위터는 우퍼의 중심부에서 약간 빗겨 장착이 되어 있어야 한다. 하이임피던스 용 트랜스포머가 장착되어 8옴 뿐 아니라 70V 및 100V로 변환하여 전관방송에도 적합한 기기이어야 한다.

(2) 기기특성

[System Details]

- Effective frequency range	: 70Hz~20kHz

- Rated noise power/voltage	: 16watts/11.3volts (rms)

- Broad-band sensitivity	: 85dB SPL

- Coverage angle(-6dB)	: 130° conical(500Hz~5kHz)

- Directivity factor(Q)	: 6

- Directivity Index	: 8dB

- Maximum continuous SPL	: 97dB

- Maximum peak SPL	: 103dB

- Rated impedance	: 8ohms

- Recommended amplifier	: 32watts

- Transformer taps

70V: 16, 8, 4, 2, 1 watts

100V: 16, 8, 4, 2 watts

8ohm bypass

- LF transducer	: 100mm[4in] Polypropylene woofer

: 25mm[1in] voice-coil

- HF transducer	: 25mm[1in] Aluminium dome

tweeter

25mm[1in] voice-coil

- Input connector type	: Euroblock connector with parallel

output

- Enclosure material	: UV treated, high impact ABS

polymer

- Grille material	: Powder coated steel

- Yoke material	: Powder coated steel, brass inserts

[Enclosure Details]

- Ingress protection	: IP-44

- Operating environment	: Designed for indoor use

- Operating Temperature Range	: -20 to 50 °C [-4 to 122 °F]

- Net weight	: 2.4kg[5.3lb]

- Product dimensions	: 230 x 160 x 150 mm

[9.1 x 6.3 x 5.9 in]

- Shipping weight	: 5.3kg[11.8lb] (pair packed)

- Shipping dimensions	: 292 x 206 x 368 mm

[11.5 x 8.1 x 14.5 in]

(pair packed)

** AC-S4T 또는 동등 이상품 이어야 한다.