CEILING SUBWOOFER SPEAKER

━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━

(1) 기능

본 기기는 8인치 2웨이 천장형 스피커로 8인치 우퍼에는 다습한 환경에 강한 폴리프로필렌 콘이 장착되어 있어야 한다. 40Hz 이하의 저역 재생을 위한 대형 포트로 구현되어 있어야 하고 120Hz 로우 패스 필터를 내장하고 있어야 한다. 배플과 마운팅 탭은 강화 플라스틱으로 주조되어 있어야 하며 인클로져의 후면은 파우더 코팅이 된 두터운 강철이 적용되어 있어야 한다. 하이임피던스 용 트랜스포머가 장착되어 8옴 뿐 아니라 70V 및 100V로 변환하여 전관방송에도 적합한 기기이어야 한다.

(2) 기기특성

- Configuration	: Ceiling subwoofer, ported

- Low-frequency transducer	: 8"(20cm) weather resistant,

polypropylene cone woofer,

rubber surround

- Frequency range

Frequency response(-6dB)	: 39Hz~184Hz

Useable frequency range(-10dB)	: 28Hz~208Hz

- Filter	: 120Hz low-pass, passive,

bypassable

- Maximum output

Calculated peak output	: 118dB SPL

Calculated continuous output	: 112dB SPL

- Nominal impedance	: 8Ω

- Power rating

RMS power handling	: 100W(100 hours IEC)

Recommended max amp power	: 200W RMS

- Sensitivity	: 92dB, 2.83V, 1m, free space(4π)

- Transformers

Type	: Custom low distortion laminated

core, wide bandwidth design

Taps	: 70V; 60, 30, 15, 7.5 W/

100V; 60, 30, 15 W/

8Ω selected by switch

- Environmental	: Exceeds Mil Spec 810 for humidity,

salt spray and dust; IEC 60529

IP-X3 splash rating

- Enclosure

Material	: Injection molded, high impact

polystyrene baffle on a steel

enclosure

Finish	: White(paintable)

Grille	: Painted aluminum

Connectors	: Ceramic block or 4-pin Euro

terminals in fire protective

sub-chamber

Mounting Hardware	: Rails and C-ring for ceiling tile

installation

Weight – Net/Shipping	: 20lb(9.1kg)/28lb(12.7kg)

** AD-C81Tw 또는 동등 이상품 이어야 한다.