CEILING SPEAKER

━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━

(1) 기능

본 기기는 12인치 천정형 우퍼로서 음악 플레이백, PA용도로 제작되어야 하고 높은 출력을 필요로 하는 상황에 적합하여야 한다. 트랜스듀서와 크로스오버 네트워크를 사용하여야 하고 스틸 배플로 마운팅 된 동축 트랜스듀서를 포함하여야 하며 하이임피던스 용 트랜스포머가 장착되어 16옴 뿐 아니라 70V 및 100V로 변환하여 전관방송에도 적합한 기기이어야 한다.

(2) 기기특성

- Configuration	: Passive

- Transducers

Low-frequency	: 12"(304mm) ferrite woofer

High-frequency	: 1.75"(44mm) neodymium

compression driver

- Frequency range

Frequency response(-6dB)	: 42Hz~18kHz

Useable frequency range(-10dB)	: 37Hz~18kHz

- Maximum output

Calculated peak output	: 124dB SPL

Calculated continuous output	: 118dB SPL

- Nominal coverage	: 85° horizontal and vertical

- Nominal impedance	: 16Ω

- Power Rating

RMS power handling	: 300W

Recommended max amp power	: 600W

- Sensitivity	: 93dB SPL, 1W/1m

- Bass loading	: Ported

- Transformer

Type	: Custom low distortion laminated

core, wide bandwidth design

Taps	: 100V; 16Ω bypass, 150W, 75W,

37.5W

70V: 16Ω bypass, 150W, 75W,

37.5W, 18.2W

- Enclosure Volume	: 88L(3.1ft3)

- Enclosure

Connectors	: Back box; ceramic block connector

inputs and “through” connectors

(rated for 400W max).

Loudspeaker baffle; Euro-style

connectors.

Mounting Hardware	: Pre-installed, suspended, back box,

four mounting tabs.

Loudspeaker baffle; six mounting

screws.

Weight – Net	: 25lb/11.3kg

Back box; 53lb/24kg

Complete assembly; 78lb/35.3kg

- Dimensions(HWD)	: Complete assembly;

23" x 18" x 15.5“

(584mm x 454mm x 393mm)

** AD-C1200 또는 동등 이상품 이어야 한다.