CEILING SPEAKER

━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━

(1) 기능

본 기기는 8인치 천정형 우퍼로서 음악 플레이백, PA용도로 제작되어야 하고 높은 출력을 필요로 하는 상황에 적합하여야 한다. 트랜스듀서와 크로스오버 네트워크를 사용하여야 하고 스틸 배플로 마운팅 된 동축 트랜스듀서를 포함하여야 하며 하이임피던스 용 트랜스포머가 장착되어 16옴 뿐 아니라 70V 및 100V로 변환하여 전관방송에도 적합한 기기이어야 한다.

(2) 기기특성

- Configuration	: Passive

- Transducers

Low-frequency	: 8"(203mm) ferrite woofer

High-frequency	: 1.4"(36mm) neodymium

compression driver

- Frequency range

Frequency response(-6dB)	: 61Hz~18kHz

Useable frequency range(-10dB)	: 52Hz~18kHz

- Maximum output

Calculated peak output	: 120dB SPL

Calculated continuous output	: 114dB SPL

- Nominal coverage	: 90° horizontal and vertical

- Nominal impedance	: 16Ω

- Power rating

RMS power handling	: 200W

Recommended max amp power	: 400W

- Sensitivity	: 91dB SPL, 1W/1m

- Bass loading	: Ported

- Transformers

Type	: Custom low distortion laminated

core, wide bandwidth design

Taps	: 100V; 16Ω bypass, 100W, 50W,

25W

70V; 16Ω bypass, 100W, 50W,

25W, 12.5W

- Enclosure Volume	: 18L(0.64ft3)

- Enclosure

Connectors	: Two 2-pin Euro-style connectors

Mounting Hardware	: Captive, integral Mounting Clamps.

Insert enclosure into mounting

hole, and tighten. Suspended

ceiling Split-ring and Suspended

Ceiling Tile Rails - sold separately.

- Weight - Net	: 16lb(7.3kg)

- Dimensions	: Diameter; 13.4"(340mm)

Depth; 11.9"(302mm)

** AD-C821 또는 동등 이상품 이어야 한다.